DICOM PS3.16 2020a - Content Mapping Resource

CID 3337 Hemodynamic Annotations (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 3337 Hemodynamic Annotations

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20160314

UID:

  1.2.840.10008.6.1.63

Table CID 3337. Hemodynamic Annotations

Coding Scheme Designator | Code Value | Code Meaning | SNOMED-RT ID | UMLS Concept Unique ID
--- | --- | --- | --- | ---
DCM | 109014 | 35% of thermal/dye dilution CO |  |
DCM | 109015 | 70% of thermal/dye dilution CO |  |
DCM | 109016 | A wave peak pressure |  |
DCM | 109017 | A wave pressure, average |  |
DCM | 109018 | Beat detected (accepted) |  |
DCM | 109019 | Beat detected (rejected) |  |
SCT | 314453003 | Average diastolic blood pressure | F-00E22 | C1282163
SCT | 314451001 | Minimum diastolic blood pressure | F-00E1F | C1282161
SCT | 416190007 | End diastole | R-FAB5C | C1562146
DCM | 109023 | End of expiration |  |
DCM | 109024 | End of inspiration |  |
DCM | 109070 | End of systole |  |
DCM | 109071 | Indicator mean transit time |  |
DCM | 109025 | Max dp/dt |  |
DCM | 109026 | Max neg dp/dt |  |
SCT | 6797001 | Mean blood pressure | F-31150 | C0428886
DCM | 109028 | Peak of thermal cardiac output bolus |  |
DCM | 109029 | Start of expiration |  |
DCM | 109030 | Start of inspiration |  |
DCM | 109031 | Start of thermal CO |  |
SCT | 314440001 | Average systolic blood pressure | F-00E14 | C1282151
SCT | 314439003 | Maximum systolic blood pressure | F-00E11 | C1282150
DCM | 109072 | Tau |  |
DCM | 109073 | V max myocardial |  |
DCM | 109034 | V wave peak pressure |  |
DCM | 109035 | V wave pressure, average |  |
DCM | 109036 | Valve close |  |
DCM | 109037 | Valve open |  |

Prev | Up | Next
CID 3335 ECG Annotations | Home | CID 3339 Electrophysiology Annotations

DICOM PS3.16 2020a - Content Mapping Resource