DICOM PS3.16 2020a - Content Mapping Resource

CID 3690 ECG Control Variables Numeric (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 3690 ECG Control Variables Numeric

This Context Group includes the ECG control variables specified in the ISO/IEEE 11073-10102 nomenclature that take numeric values. The terms are included in the table below for reference; these may not constitute the complete current list (see the ISO/IEEE Standard).

### Note

Codes reprinted by permission of IEEE, Copyright 2004 by IEEE. ISO/IEEE 11073-10102 available through http://standards.ieee.org/.

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20110330

UID:

  1.2.840.10008.6.1.895

Table CID 3690. ECG Control Variables Numeric

Coding Scheme Designator | Code Value | Code Meaning | ISO/IEEE 11073 MDC Equivalent Reference ID (Informative)
--- | --- | --- | ---
MDC | 10:11393 | Sample rate | MDC_ECG_CTL_VBL_SAMPLE_RATE
MDC | 10:11394 | Sensitivity | MDC_ECG_CTL_VBL_SENSITIVITY
MDC | 10:11395 | Zero offset | MDC_ECG_CTL_VBL_ZERO_OFFSET
MDC | 10:11397 | Pad value | MDC_ECG_CTL_VBL_PAD_VALUE
MDC | 10:11398 | Time skew | MDC_ECG_CTL_VBL_TIME_SKEW
MDC | 10:11399 | Sample skew | MDC_ECG_CTL_VBL_SAMPLE_SKEW
MDC | 10:11400 | Time offset | MDC_ECG_CTL_VBL_TIME_OFFSET
MDC | 10:11403 | Low pass filter cutoff freq | MDC_ECG_CTL_VBL_ATTR_FILTER_CUTOFF_FREQ
MDC | 10:11408 | Notch filter frequency | MDC_ECG_CTL_VBL_ATTR_FILTER_NOTCH_FREQ
MDC | 10:11409 | Notch filter bandwidth | MDC_ECG_CTL_VBL_ATTR_FILTER_NOTCH_BANDWIDTH
MDC | 10:11418 | Interpolator SNR | MDC_ECG_CTL_VBL_INTERPOLATOR_SNR

Prev | Up | Next
CID 3689 ECG Global Waveform Durations | Home | CID 3691 ECG Control Variables Text

DICOM PS3.16 2020a - Content Mapping Resource