DICOM PS3.3 2020a - Information Object Definitions

C.8.19.6.6 X-Ray Calibration Device Usage Macro (Current)
Prev | C.8.19.6 Enhanced XA/XRF Image Functional Group Macros | Next

##### C.8.19.6.6 X-Ray Calibration Device Usage Macro

Table C.8.19.6-6 specifies the Attributes containing the X-Ray Calibration Device Usage Functional Group Macro.

Table C.8.19.6-6. X-Ray Calibration Device Usage Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Calibration Sequence | (0018,9455) | 1 | Sequence containing the calibration flag for this frame. Only a single Item shall be included in this Sequence.
>Calibration Image | (0050,0004) | 1 | Indicates whether a reference object (phantom) of known size is present in the frame and was used for calibration. Enumerated Values: YES NO ### Note Device is identified using the Device Module. See Section C.7.6.12.

Prev | Up | Next
C.8.19.6.5 X-Ray Frame Detector Parameters Macro | Home | C.8.19.6.7 X-Ray Object Thickness Macro

DICOM PS3.3 2020a - Information Object Definitions