DICOM PS3.3 2020a - Information Object Definitions

C.36.2.2.3 RT Accessory Device Identification Macro (Current)
Prev | C.36.2.2 RT Second Generation Device Macros | Next

##### C.36.2.2.3 RT Accessory Device Identification Macro

The RT Accessory Device Identification Macro identifies an RT accessory device and its location.

Table C.36.2.2.3-1. RT Accessory Device Identification Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Include Table 10.35-1 “Device Model Macro Attributes”.
Include Table 10.36-1 “Device Identification Macro Attributes”. | CID is defined by invocation.
RT Accessory Device Slot ID | (300A,0615) | 2C | Identifier for location (slot) of radiation modifier accessory where the current accessory is inserted. Required if accessory is located in a slot and Referenced RT Accessory Holder Device Index (300A,060E) is not present.
RT Accessory Slot Distance | (300A,0613) | 2C | Distance in mm from the reference location as specified by RT Device Distance Reference Location Code Sequence (300A,0659) to the Accessory Slot. Required if RT Accessory Device Slot ID (300A,0615) is present and has a value.
Referenced RT Accessory Holder Device Index | (300A,060E) | 2C | The value of Device Index (3010,0039) of the Accessory Holder device in the RT Accessory Holder Definition Sequence (300A,0614). Required if accessory is mounted on a holder device and RT Accessory Device Slot ID (300A,0615) is not present.
RT Accessory Holder Slot ID | (300A,0611) | 2C | Identifier for location (slot) of radiation modifier in the Accessory Holding device where the current accessory is inserted. Required if Referenced RT Accessory Holder Device Index (300A,060E) is present and has a value and the referenced Accessory Holder Device contains an RT Accessory Holder Slot Sequence (300A,0610).

Prev | Up | Next
C.36.2.2.2 RT Patient Support Devices Macro | Home | C.36.2.2.4 RT Treatment Position Macro

DICOM PS3.3 2020a - Information Object Definitions