DICOM PS3.3 2020a - Information Object Definitions

A.65 Ophthalmic Visual Field Static Perimetry Measurements IOD (Current)
Prev | A Composite Information Object Definitions (Normative) | Next

## A.65 Ophthalmic Visual Field Static Perimetry Measurements IOD

### A.65.1 Ophthalmic Visual Field Static Perimetry Measurements IOD Description

The Ophthalmic Visual Field Static Perimetry Measurements IOD is used to encode results of static perimetry with visual field devices.

Prev | Up | Next
A.64.4 RT Beams Delivery Instruction IOD Content Constraints | Home | A.65.2 Ophthalmic Visual Field Static Perimetry Measurements IOD Entity-Relationship Model

DICOM PS3.3 2020a - Information Object Definitions