DICOM PS3.11 2020a - Media Storage Application Profiles

A.3.4 Other Parameters (Current)
Prev | A.3 STD-XABC-CD Basic Cardiac Profile | Next

### A.3.4 Other Parameters

This section defines other parameters common to all specific Application Profiles in the STD-XABC class that need to be specified in order to ensure interoperable media interchange.

#### A.3.4.1 Image Attribute Values

The attributes listed in Table A.3-3 used within the X-Ray Angiographic Image files shall take the values specified.

Table A.3-3. STD-XABC-CD- Required Image Attribute Values

Attribute | Tag | Value
--- | --- | ---
Modality | (0008,0060) | XA
Rows | (0028,0010) | 512 (see below)
Columns | (0028,0011) | 512 (see below)
Bits Allocated | (0028,0100) | 8
Bits Stored | (0028,0101) | 8

When creating or updating a File-set, Rows or Columns shall not exceed a value of 512. When reading a File-set, an FSR or FSU shall accept a value of at least 512 for Rows or Columns.

Overlay data, if present, shall be encoded in Overlay Data (60XX,3000).

##### A.3.4.1.1 Attribute Value Precedence

Retired. See PS3.11 2004.

### Note

The retired Detached Patient Management SOP Class was previously suggested to allow patient identification and demographic information to be updated without changing the composite Image IOD files. This usage is now retired.

Prev | Up | Next
A.3.3.2 Icon Images | Home | B 1024 X-Ray Angiographic Application Profile (Normative)

DICOM PS3.11 2020a - Media Storage Application Profiles