DICOM PS3.17 2020a - Explanatory Information

PPPP.8.2 Streaming DICOM-RTV From Stored IOD (Current)
Prev | PPPP.8 Storage Considerationa | Next

### PPPP.8.2 Streaming DICOM-RTV From Stored IOD

Regarding initiating a DICOM-RTV stream from a stored instance, the application should be able to regenerate the different DICOM-RTV flows, with the same synchronization characteristics, in compliance with SMPTE ST 2110-10.

- Subcase 1 is conventional video IODs e.g., ultrasound video/multi-frame or angio video/multi-frame.

- Subcase 2 is one or more video IODs that were previously DICOM-RTV, e.g., stored like PPPP.8.1.

- If the multiple stored IOD of the subcase 2 contain synchronization information extracted from DICOM, it should be possible to playback them with a good synchronization.

Prev | Up | Next
PPPP.8 Storage Considerationa | Home | PPPP.9 Example of Engineering Implementation

DICOM PS3.17 2020a - Explanatory Information