DICOM PS3.2 2020a - Conformance

B.8.4 Grayscale Image Consistency (Current)
Prev | B.8 Annexes | Next

### B.8.4 Grayscale Image Consistency

The high resolution display monitor attached to EXAMPLEINTEGRATED-MODALITY can be calibrated according to the Grayscale Standard Display Function (GSDF). The Service/Installation Tool is used together with a luminance meter to measure the Characteristic Curve of the display system and the current ambient light. See the EXAMPLE-INTEGRATED-MODALITY Service Manual for details on the calibration procedure and supported calibration hardware. The result of the calibration procedure is a Monitor Correction LUT that will be active within the display subsystem after a system reboot.

Prev | Up | Next
B.8.3 Coded Terminology and Templates | Home | B.8.5 Standard Extended / Specialized / Private SOP Classes

DICOM PS3.2 2020a - Conformance