DICOM PS3.7 2020b - Message Exchange

C.5.12 Invalid SOP Instance (Current)
Prev | C.5 Failure Status Class | Next

### C.5.12 Invalid SOP Instance

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0117H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the SOP Instance UID that violated the UID construction rules.

Prev | Up | Next
C.5.11 Invalid Attribute Value | Home | C.5.13 Missing Attribute

DICOM PS3.7 2020b - Message Exchange