DICOM PS3.16 2020b - Content Mapping Resource

TID 3101 Image Acquisition (Current)
Prev | Procedure Log IOD Templates | Next

### TID 3101 Image Acquisition

The Image Acquisition Template allows recording of the essential parameters of a digital image acquired during the procedure.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3101. Image Acquisition

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | IMAGE | EV (121138, DCM, "Image Acquired") | 1 | M |  |
2 | > | HAS ACQ CONTEXT | UIDREF | EV (112002, DCM, "Series Instance UID") | 1 | M |  |
3 | > | HAS ACQ CONTEXT | CODE | EV (121139, DCM, "Modality") | 1 | M |  | DCID 29 “Acquisition Modality” Derived from referenced image SOP Instance attribute (0008,0060)
4 | > | HAS PROPERTIES | NUM | EV (121140, DCM, "Number of Frames") | 1 | U |  |
5 | > | HAS PROPERTIES | TEXT | EV (121141, DCM, "Image Type") | 1 | U |  | From referenced image SOP Instance attribute (0008,0008)
6 | > | HAS ACQ CONTEXT | NUM | EV (112011, DCM, "Positioner Primary Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
7 | > | HAS ACQ CONTEXT | NUM | EV (112012, DCM, "Positioner Secondary Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
8 | > |  | INCLUDE | DTID 3010 “Log Entry Qualifiers” | 1 | U |  |

Prev | Up | Next
TID 3100 Procedure Action | Home | TID 3102 Waveform Acquisition

DICOM PS3.16 2020b - Content Mapping Resource