DICOM PS3.4 2020b - Service Class Specifications

DD.3.2.2 N-GET (Current)
Prev | DD.3.2 DIMSE Service Group | Next

#### DD.3.2.2 N-GET

The N-GET is used to get the verification status and results of the applicable Machine Verification SOP Class.

##### DD.3.2.2.1Verification Parameters Selector Attribute Macro

Table DD.3.2.2.1-1 describes N-GET support requirements for the Selector Attribute Macro. See Section 5.4 for requirements type code meaning.

Table DD.3.2.2.1-1. Verification Parameters Selector Attribute Macro

Attribute Name | Tag | Req. Type N-GET (SCU/SCP)
--- | --- | ---
Selector Attribute | (0072,0026) | -/1
Selector Value Number | (0072,0028) | -/1
Selector Sequence Pointer | (0072,0052) | -/1
Selector Sequence Pointer Private Creator | (0072,0054) | -/1
Selector Sequence Pointer Items | (0074,1057) | -/1
Selector Attribute Private Creator | (0072,0056) | -/1

Prev | Up | Next
DD.3.2 DIMSE Service Group | Home | DD.3.2.2.2 Attributes

DICOM PS3.4 2020b - Service Class Specifications