DICOM PS3.2 2020b - Conformance

L.4.4 Configuration (Current)
Prev | L Conformance Statement Sample DICOM-RTV Service Provider (Informative) | Next

## L.4.4 Configuration

### L.4.4.1 DICOM-RTV Interface

The EXAMPLE-RTV-SERVICE is configured to define the following parameters expressed in the SDP object:

- the RTP payload type (PT) used for the video is 96

- the RTP payload type (PT) used for DICOM-RTV Metadata is 104.

Prev | Up | Next
L.4.3.3 IPv4 and IPv6 Support | Home | L.5 Media Interchange

DICOM PS3.2 2020b - Conformance