DICOM PS3.3 2020b - Information Object Definitions

C.8.8.15.12 Nominal Thickness and Nominal Transmission (Current)
Prev | C.8.8.15 RT Brachy Application Setups Module | Next

##### C.8.8.15.12 Nominal Thickness and Nominal Transmission

If provided, Source Encapsulation Nominal Thickness (300A,0222), Brachy Accessory Device Nominal Thickness (300A,026A), Source Applicator Wall Nominal Thickness (300A,029C), and Channel Shield Nominal Thickness (300A,02B8) shall indicate that the related objects are of uniform thickness with the specified value. If this is not the case, these Attributes shall not be provided.

If provided, Source Encapsulation Nominal Transmission (300A,0224), Brachy Accessory Device Nominal Transmission (300A,026C), Source Applicator Wall Nominal Transmission (300A,029E), and Channel Shield Nominal Transmission (300A,02BA) shall indicate that the related objects are of uniform transmission with the specified value. If this is not the case, these Attributes shall not be provided.

No assumptions are made about the source characteristics beyond the parameters specified here.

Prev | Up | Next
C.8.8.15.11 Cumulative Dose Reference Coefficient | Home | C.8.8.15.13 Reference Point for Calibration of Beta Emitting Isotopes

DICOM PS3.3 2020b - Information Object Definitions