DICOM PS3.7 2020b - Message Exchange

C.5 Failure Status Class (Current)
Prev | C Status Type Encoding (Normative) | Next

## C.5 Failure Status Class

Statuses in this Status Class convey that the operation/notification failed and was not performed.

### C.5.1 Error: Cannot understand

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Offending Element | (0000,0901) | AT | 1-n | This optional field contains a list of the elements in which the error was detected.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

Prev | Up | Next
C.4.3 Attribute Value out of range | Home | C.5.2 Error: Data Set does not match SOP Class

DICOM PS3.7 2020b - Message Exchange