DICOM PS3.3 2020b - Information Object Definitions

A.76.4 Wide Field Ophthalmic Photography Stereographic Projection Image IOD Content Constraints (Current)
Prev | A.76 Wide Field Ophthalmic Photography Stereographic Projection Image IOD | Next

### A.76.4 Wide Field Ophthalmic Photography Stereographic Projection Image IOD Content Constraints

The following constraints on Series and Image Attributes take precedence over the descriptions given in the Module Attribute Tables.

#### A.76.4.1 Bits Allocated, Bits Stored, and High Bit

These Attributes shall be determined based upon the Photometric Interpretation (0028,0004):

Photometric Interpretation (0028,0004) | Bits Allocated (0028,0100) | Bits Stored (0028,0101) | High Bit (0028,0102)
--- | --- | --- | ---
MONOCHROME2 | 8 | 8 | 7
16 | 16 | 15
RGB YBR_FULL_422 YBR_PARTIAL_420 YBR_ICT YBR_RCT | 8 | 8 | 7

Prev | Up | Next
A.76.3 Wide Field Ophthalmic Photography Stereographic Projection Image IOD Modules | Home | A.76.4.2 Contrast/Bolus Agent Sequence

DICOM PS3.3 2020b - Information Object Definitions