DICOM PS3.17 2020b - Explanatory Information

S.5.4 Description of This Device (Current)
Prev | S.5 Adding The First Managed Device to A Legacy Network | Next

### S.5.4 Description of This Device

This device needs its own LDAP entry. This is used during the system start up process. The LDAP server updates must be performed.

Prev | Up | Next
S.5.3.4 Descriptions of Other Devices | Home | S.6 Switching A Node From Unmanaged to Managed in A Mixed Network

DICOM PS3.17 2020b - Explanatory Information