DICOM PS3.4 2020b - Service Class Specifications

H.3.2.2 Meta SOP Class Definitions (Current)
Prev | H.3.2 Print Management Meta SOP Classes | Next

#### H.3.2.2 Meta SOP Class Definitions

##### H.3.2.2.1 Basic Grayscale Print Management Meta SOP Class

The Meta SOP Class is defined by the following set of supported SOP Classes.

Table H.3.2.2.1-1. SOP Classes of Basic Grayscale Print Management Meta SOP Class

SOP Class Name | Reference | Usage SCU/SCP
--- | --- | ---
Basic Film Session SOP Class | H.4.1 | M/M
Basic Film Box SOP Class | H.4.2 | M/M
Basic Grayscale Image Box SOP Class | H.4.3.1 | M/M
Printer SOP Class | H.4.6 | M/M

### Note

The image pixel data are part of the Basic Grayscale Image Box SOP Class

The meaning of the Usage SCU/SCP is described in Section H.2.4.

The Basic Grayscale Print Management Meta SOP Class UID has the value "1.2.840.10008.5.1.1.9".

Prev | Up | Next
H.3.2 Print Management Meta SOP Classes | Home | H.3.2.2.2 Basic Color Print Management Meta SOP Class

DICOM PS3.4 2020b - Service Class Specifications