DICOM PS3.16 2020b - Content Mapping Resource

TID 3713 ECG Global Measurements (Current)
Prev | ECG Report Templates | Next

### TID 3713 ECG Global Measurements

The ECG Global Measurements Template provides a structure for measurements calculated across the ECG waveform as a whole (multiple leads).

As an Extensible Template, applications may include any ECG global measurements, such as angles of the electrical vector of various ECG waves. The recommended vocabulary for such concepts is ISO/IEEE 11073-10102.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3713. ECG Global Measurements

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (122158, DCM, "ECG Global Measurements") | 1 | M |  |
2 | > | HAS OBS CONTEXT | INCLUDE | DTID 3715 “ECG Measurement Source” | 1 | U |  |
3 | > | CONTAINS | NUM | DT (2:16020, MDC, "Atrial Heart Rate") | 1 | U |  | UNITS = EV ({H.B.}/min, UCUM, "BPM")
4 | > | CONTAINS | NUM | DT (2:16016, MDC, "Ventricular Heart Rate") | 1 | M |  | UNITS = EV ({H.B.}/min, UCUM, "BPM")
5 | > | CONTAINS | NUM | DT (2:16160, MDC, "QT interval global") | 1 | M |  | UNITS = EV (ms, UCUM, "ms")
6 | > | CONTAINS | NUM | DT (2:15876, MDC, "QTc interval global") | 1 | U |  | UNITS = EV (ms, UCUM, "ms")
7 | >> | HAS PROPERTIES | CODE | DT (111001, DCM, "Algorithm Name") | 1 | U |  | DCID 3678 “QT Correction Algorithms”
8 | > | CONTAINS | NUM | DT (2:15872, MDC, "PR interval global") | 1 | M |  | UNITS = EV (ms, UCUM, "ms")
9 | > | CONTAINS | NUM | DT (2:16156, MDC, "QRS duration global") | 1 | M |  | UNITS = EV (ms, UCUM, "ms")
10 | > | CONTAINS | NUM | DT (2:16168, MDC, "RR interval global") | 1 | M |  | UNITS = EV (ms, UCUM, "ms")
11 | > | CONTAINS | NUM | DCID 3689 “ECG Global Waveform Durations” | 1-n | U |  | UNITS = EV (ms, UCUM, "ms")
12 | > | CONTAINS | NUM | DCID 3229 “ECG Axis Measurements” | 1-n | U |  | UNITS = EV (deg, UCUM, "deg")
13 | > | CONTAINS | NUM | DT (2:16032, MDC, "Count of all beats") | 1 | U |  | UNITS = EV ({beats}, UCUM, "beats")
14 | > | CONTAINS | NUM | DT (122707, DCM, "Number of Ectopic Beats") | 1 | U |  | UNITS = EV ({beats}, UCUM, "beats")
15 | >> | HAS PROPERTIES | CODE | EV (116676008, SCT, "Associated Morphology") | 1-n | U |  | BCID 3234 “Ectopic Beat Morphology”

Prev | Up | Next
TID 3708 ECG Waveform Information | Home | TID 3714 ECG Lead Measurements

DICOM PS3.16 2020b - Content Mapping Resource