DICOM PS3.17 2020b - Explanatory Information

XXX.3.10.3.4 Render Display Module Recommendations (Current)
Prev | XXX.3.10.3 Encoding Details | Next

##### XXX.3.10.3.4 Render Display Module Recommendations

Table XXX.3.10.3.4-1. Render Display Module Recommendations

Attribute Name | Tag | Comment
Pixel Presentation | (0008,9205) | Set to "TRUE_COLOR"
Volume Stream Sequence | (0070,1A08) |
Item #1 of Volume Stream Sequence
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1, referencing the first item in the Volumetric Presentation Input Set Sequence (0070,120A)
>Presentation State Classification Component Sequence | (0070,1801) |
>Item #1 of Presentation State Classification Component Sequence
>>Component Type | (0070,1802) | Set to ONE_TO_RGBA
>>Component Input Sequence | (0070,1803) |
>>Item #1 of Component Input Sequence
>>>Volumetric Presentation Input Index | (0070,1804) | Set to 1 referencing the first item in Volumetric Presentation State Input Sequence (0070,1201)
>>RGB LUT Transfer Function | (0028,140F) | Set to TABLE
>>Alpha LUT Transfer Function | (0028,1410) | Set to TABLE
>>RGB Palette Color Lookup Table Descriptors and Data
>>Alpha Palette Color Lookup Table Descriptor and Data
Presentation State Compositor Component Sequence | (0070,1805) | empty
ICC Profile | (0028,2000) | Value corresponding to IEC 61966-2-1:1999
Color Space | (0028,2002) | Set to SRGB

Prev | Up | Next
XXX.3.10.3.3 Render Shading Module Recommendations | Home | XXX.3.10.3.5 Volumetric Graphic Annotation Module Recommendations

DICOM PS3.17 2020b - Explanatory Information