DICOM PS3.5 2020b - Data Structures and Encoding

10.15 Transfer Syntax for SMPTE ST 2110-20 Uncompressed Progressive Active Video (Current)
Prev | 10 Transfer Syntax | Next

## 10.15 Transfer Syntax for SMPTE ST 2110-20 Uncompressed Progressive Active Video

This Transfer Syntax is used for Uncompressed Video pixels carried in a DICOM-RTV Flow (separated from DICOM-RTV Metadata Flow) as described by [SMPTE ST 2110-20], in the case the video is progressive (e.g., 1080p). The main parameters of the transfer syntax are described in Section A.8.

Prev | Up | Next
10.14 Transfer Syntax for HEVC/H.265 Main 10 Profile / Level 5.1 Video Compression | Home | 10.16 Transfer Syntax for SMPTE ST 2110-20 Uncompressed Interlaced Active Video

DICOM PS3.5 2020b - Data Structures and Encoding