DICOM PS3.2 2020b - Conformance

I.4.4 Configuration (Current)
Prev | I.4 Networking | Next

### I.4.4 Configuration

#### I.4.4.1 HTTP URI Interface

The EXAMPLE-WADO-SERVICE can be configured to respond on two ports, one for unprotected HTTP traffic and one for TLS protected traffic. The TLS port will refuse any connection from a system that is not recognized as authenticated by a known authority.

Prev | Up | Next
I.4.3.3 IPv4 and IPv6 Support | Home | I.4.4.2 WS Interface

DICOM PS3.2 2020b - Conformance