DICOM PS3.3 2020c - Information Object Definitions

A.8.5 Multi-frame True Color Secondary Capture Image IOD (Current)
Prev | A.8 Secondary Capture Image IOD | Next

### A.8.5 Multi-frame True Color Secondary Capture Image IOD

#### A.8.5.1 Multi-frame True Color Image IOD Description

The Multi-frame True Color Secondary Capture (SC) Image Information Object Definition (IOD) specifies True Color images that are converted from a non-DICOM format to a modality independent DICOM format.

This IOD is typically used for screen captured or synthetic images where true color is used, but may also be appropriate for scanned color documents.

Prev | Up | Next
A.8.4.5 Multi-frame Grayscale Word SC Image Functional Group Macros | Home | A.8.5.2 Multi-frame True Color SC Image IOD Entity-Relationship Model

DICOM PS3.3 2020c - Information Object Definitions