DICOM PS3.11 2020c - Media Storage Application Profiles

C.5 Combined Calibration (CC) Class Requirements (Current)
Prev | C Ultrasound Application Profile (Normative) | Next

## C.5 Combined Calibration (CC) Class Requirements

All implementations conforming to the Application Profile Class CC shall include the US Region Calibration Module including the pixel component organization data element (0018,6044) and other data elements that are conditional on that data element.

Prev | Up | Next
C.4 Spatial Calibration (SC) Class Requirements | Home | D General Purpose CD-R, DVD and BD Interchange Profiles (Normative)

DICOM PS3.11 2020c - Media Storage Application Profiles