DICOM PS3.3 2020c - Information Object Definitions

C.8.19.6.7 X-Ray Object Thickness Macro (Current)
Prev | C.8.19.6 Enhanced XA/XRF Image Functional Group Macros | Next

##### C.8.19.6.7 X-Ray Object Thickness Macro

Table C.8.19.6-7 specifies the Attributes containing the X-Ray Object Thickness Group Macro.

Table C.8.19.6-7. X-Ray Object Thickness Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Object Thickness Sequence | (0018,9456) | 1 | Sequence containing object thickness for this frame. Only a single Item shall be included in this Sequence.
>Calculated Anatomy Thickness | (0018,9452) | 1 | The physical thickness in mm of the anatomic region of interest as specified in the Anatomic Region Sequence (0008,2218) in the direction of the center of the beam. ### Note The value takes in account the position relative to object and the X-Ray source - detector axis.

Prev | Up | Next
C.8.19.6.6 X-Ray Calibration Device Usage Macro | Home | C.8.19.6.8 X-Ray Frame Acquisition Macro

DICOM PS3.3 2020c - Information Object Definitions