DICOM PS3.5 2020c - Data Structures and Encoding

A.7 DICOM JPIP Referenced Deflate Transfer Syntax (Explicit VR) (Current)
Prev | A Transfer Syntax Specifications (Normative) | Next

## A.7 DICOM JPIP Referenced Deflate Transfer Syntax (Explicit VR)

This Transfer Syntax applies to the encoding of the entire DICOM Data Set.

The entire Data Set is first encoded according to the rules specified in Section A.6.

The entire byte stream is then compressed using the "Deflate" algorithm defined in Internet RFC 1951.

This DICOM JPIP Referenced Deflate Transfer Syntax shall be identified by a UID of Value "1.2.840.10008.1.2.4.95".

Prev | Up | Next
A.6 DICOM JPIP Referenced Transfer Syntax (Explicit VR) | Home | A.8 SMPTE ST 2110-20 Uncompressed Progressive Active Video Transfer Syntax

DICOM PS3.5 2020c - Data Structures and Encoding