DICOM PS3.4 2020c - Service Class Specifications

EE.2.3 SOP Class Definitions and UIDs (Current)
Prev | EE.2 Display System SOP Class | Next

### EE.2.3 SOP Class Definitions and UIDs

The SOP Class UID of the Display System SOP Class shall have the value of "1.2.840.10008.5.1.1.40".

Prev | Up | Next
EE.2.2 DIMSE Service Group | Home | EE.2.4 Reserved Identifications

DICOM PS3.4 2020c - Service Class Specifications