DICOM PS3.2 2020c - Conformance

B.4.4.2 Parameters (Current)
Prev | B.4.4 Configuration | Next

#### B.4.4.2 Parameters

A large number of parameters related to acquisition and general operation can be configured using the Service/Installation Tool. The Table below only shows those configuration parameters relevant to DICOM communication. See the EXAMPLEINTEGRATED-MODALITY Service Manual for details on general configuration capabilities.

Table B.4.4-10. Configuration Parameters Table

Parameter | Configurable (Yes/No) | Default Value
--- | --- | ---
General Parameters
Max PDU Receive Size | Yes | 65536 Bytes(64 kB)
Max PDU Send Size(larger PDUs will never be sent, even if the receiver supports a larger Max PDU Receive Size. If the receiver supports a smaller Max PDU Receive Size then the Max PDU Send Size will be reduced accordingly for the duration of the Association. Max PDU Receive Size information is exchanged during DICOM Association Negotiation in the Maximum Length Sub-Item of the A-ASSOCIATION-RQ and A-ASSOCIATE-AC) | No | 65536 Bytes(64 kB)
Time-out waiting for a acceptance or rejection response to an Association Request (Application Level Timeout) | Yes | 15 s
Time-out waiting for a response to an Association release request (Application Level Timeout) | Yes | 30 s
Time-out waiting for completion of a TCP/IP connect request (Low-level timeout) | Yes | 15 s
Time-out awaiting a Response to a DIMSE Request (Low-Level Timeout) | Yes | 360 s
Time-out for waiting for data between TCP/IP-packets (Low Level Timeout) | Yes | 30 s
Storage Parameters
Storage SCU time-out waiting for a response to a C-STORE-RQ | Yes | 120 s
Number of times a failed send job may be retried | Yes | 0 (Failed send jobs are not retried)
Delay between retrying failed send jobs | Yes | 60 s
Maximum number of simultaneously initiated Associations by the Storage AE | Yes | 1
Supported Transfer Syntaxes (separately configurable for each remote AE) | Yes | Implicit VR Little Endian Explicit VR Little Endian
Storage Commitment Parameters
Timeout waiting for a Storage Commitment Notification (maximum duration of applicability for a Storage Commitment Transaction UID). | Yes | 24 hours
Maximum number of simultaneously accepted Associations by the Storage AE | Yes | 5
Delay association release after sending a Storage Commitment Request (wait for a Storage Commitment Notification over the same association). | Yes | 120 s
Modality Worklist Parameters
Modality Worklist SCU time-out waiting for the final response to a C-FIND-RQ | Yes | 600 s
Maximum number of Worklist Items | Yes | 100
Supported Transfer Syntaxes for Modality Worklist | Yes | Implicit VR Little Endian Explicit VR Little Endian
Delay between automatic Worklist Updates | Yes | 10 mins
Query Worklist for specific Scheduled Station AE Title | Yes | EXINTMOD_WFL
Query Worklist for specific Modality Value | Yes | RF
MPPS Parameters
MPPS SCU time-out waiting for a response to a N-CREATE-RQ | Yes | 60 s
MPPS SCU time-out waiting for a response to a N-SET-RQ | Yes | 30 s
Supported Transfer Syntaxes for MPPS | Yes | Implicit VR Little Endian Explicit VR Little Endian
Print Parameters
Print SCU time-out waiting for a response to a N-CREATE-RQ | Yes | 60 s
Print SCU time-out waiting for a response to a N-SET-RQ | Yes | 30 s
Print SCU time-out waiting for a response to a N-ACTION-RQ | Yes | 360s
Supported Transfer Syntaxes (separately configurable for each remote printer) | Yes | Implicit VR Little Endian Explicit VR Little Endian
Number of times a failed print-job may be retried | Yes | 0 (Failed send jobs are not retried)
Delay between retrying failed print-jobs | Yes | 60 s
Printer correction LUT (separately configurable for each remote printer) | Yes | Identity LUT

Prev | Up | Next
B.4.4 Configuration | Home | B.5 Media Interchange

DICOM PS3.2 2020c - Conformance