DICOM PS3.8 2020c - Network Communication Support for Message Exchange

D.2 Extended User Information Negotiation (Current)
Prev | D Use and Format of the A-ASSOCIATE User Information Parameter (Normative) | Next

## D.2 Extended User Information Negotiation

The user information parameter, of the A-ASSOCIATE primitive, can be extended to support the negotiation needs of DICOM Application Entities using the UL Service. This will result in the definition of specific user information sub-items. These sub-items shall be assigned unique item-type values registered in PS3.7.

### Note

1. The values of the Sub-Items types in the User Information Field are assigned by this Standard in the range of 51H through FFH. Sub-Item values are defined by PS3.7 and PS3.8.

2. Succeeding editions of the Standard may define additional user information Sub-Items in a manner that does not affect the semantics of previously defined Sub-Items. Association acceptors compliant to an earlier edition of the Standard are required to ignore such unrecognized user information Sub-Items and not reject an Association because of their presence.

Prev | Up | Next
D Use and Format of the A-ASSOCIATE User Information Parameter (Normative) | Home | E Usage of the P-DATA Service By the DICOM Application Entity (Normative)

DICOM PS3.8 2020c - Network Communication Support for Message Exchange