DICOM PS3.16 2020c - Content Mapping Resource

TID 10002 Accumulated X-Ray Dose (Current)
Prev | X-Ray Radiation Dose SR IOD Templates | Next

### TID 10002 Accumulated X-Ray Dose

This general Template provides detailed information on projection X-Ray dose value accumulations over several irradiation events from the same equipment (typically a study or a performed procedure step).

Table TID 10002. Parameters

Parameter Name | Parameter Usage
--- | ---
$Plane | Coded term identifying to which acquisition plane the encoded information belongs.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10002. Accumulated X-Ray Dose

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (113702, DCM, "Accumulated X-Ray Dose Data") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (113764, DCM, "Acquisition Plane") | 1 | M |  | $Plane
3 | > | CONTAINS | CONTAINER | EV (122505, DCM, "Calibration") | 1-n | MC | IFF Calibration Data is available |
4 | >> | HAS CONCEPT MOD | CODE | EV (113794, DCM, "Dose Measurement Device") | 1 | M |  | DCID 10010 “Dose Measurement Devices”
5 | >> | CONTAINS | DATETIME | EV (113723, DCM, "Calibration DateTime") | 1 | M |  |
6 | >> | CONTAINS | NUM | EV (122322, DCM, "Calibration Factor") | 1 | M |  | UNITS = EV (1, UCUM, "no units")
7 | >> | CONTAINS | NUM | EV (113763, DCM, "Calibration Uncertainty") | 1 | M |  | UNITS = EV (%, UCUM, "Percent")
8 | >> | CONTAINS | TEXT | EV (113724, DCM, "Calibration Responsible Party") | 1 | M |  |
9 | >> | CONTAINS | TEXT | EV (113720, DCM, "Calibration Protocol") | 1 | U |  |
10 | > | CONTAINS | INCLUDE | DTID 10004 “Accumulated Fluoroscopy and Acquisition Projection X-Ray Dose” | 1 | MC | IFF TID 10001 Row 4 = (113957, DCM, "Fluoroscopy-Guided Projection Radiography System") or TID 10001 Row 2 = (113704, DCM, "Projection X-Ray") and TID 10001 Row 4 is absent) |
11 | > | CONTAINS | INCLUDE | DTID 10005 “Accumulated Mammography X-Ray Dose” | 1 | MC | IFF TID 10001 Row 2 = (71651007, SCT, "Mammography") |
12 | > | CONTAINS | INCLUDE | DTID 10007 “Accumulated Total Projection Radiography Dose” | 1 | MC | IFF TID 10001 Row 4 = (113958, DCM, "Integrated Projection Radiography System") or TID (10001) Row 4 = (113957, DCM, "Fluoroscopy-Guided Projection Radiography System") or TID (10001) Row 2 = (113704, DCM, "Projection X-Ray") and TID (10001) Row 4 is absent) |
13 | > | CONTAINS | INCLUDE | DTID 10006 “Accumulated Cassette-based Projection Radiography Dose” | 1 | MC | IFF TID 10001 Row 4 = (113959, DCM, "Cassette-based Projection Radiography System") |
14 | > | CONTAINS | INCLUDE | DTID 1021 “Device Participant” | 1 | MC | Required if the irradiating device is not the recording device and the dose was accumulated on a single device. | $DeviceProcedureRole = EV (113859, DCM, "Irradiating Device")
15 | > | CONTAINS | CODE | EV (128750, DCM, "Equipment Landmark") | 1 | U |  | EV (128751, DCM, "Center of Table Head")
16 | >> | HAS PROPERTIES | NUM | EV (128752, DCM, "Equipment Landmark X Position") | 1 | M |  | UNITS = EV (mm, UCUM, "mm")
17 | >> | HAS PROPERTIES | NUM | EV (128753, DCM, "Equipment Landmark Z Position") | 1 | M |  | UNITS = EV (mm, UCUM, "mm")
18 | > | CONTAINS | CONTAINER | EV (128754, DCM, "Patient Location Fiducial") | 1-n | U |  |
19 | >> | CONTAINS | INCLUDE | DTID 400 “Reference Location” | 1 | M |  |
20 | >> | HAS PROPERTIES | NUM | EV (128756, DCM, "Equipment Landmark to Patient Fiducial Z Distance") | 1 | M |  | UNITS = EV (mm, UCUM, "mm")

Content Item Descriptions

Row 5 | Date that the calibration of the equipment's dose indicators was performed
Row 6 | Typically a value provided by the medical physicist. The recorded dose or dose area product values in this report can be multiplied by this factor to obtain estimated real-world values. ### Note It is important that this value must not be applied to the measured values before storing them in the report.
Row 7 | Value range from 0 to 100 percent. Uncertainty of the 'actual' value expressed as+/- of the mean.
Row 8 | Identifies Individual or organization responsible for calibration
Row 9 | Describes calibration protocol according to equipment standards or local guidelines.
Row 14 | The device that produced the irradiation accumulated in this Template. I.e., the X-Ray source. This is not required to be present if the information is the same as that already recorded in TID 1004 “Device Observer Identifying Attributes” encoded via the inclusion of TID 1002 “Observer Context” in TID 10001 “Projection X-Ray Radiation Dose” Row 5, which in turn may be absent if identical to the content in the Enhanced General Equipment Module, or if more than one device produced the accumulated irradiation.
Rows 16 and 17 | These coordinates relate a visible landmark on the X-Ray table to the Table Reference Point that is arbitrarily defined by the manufacturer and not necessarily visible to the operator. The Equipment Landmark Y Position is not recorded since it is, by definition, in the plane of the table as is the origin of the Table Coordinate System so the value would always be zero.
Row 19 | In many instances, the values will be either: EV (128772, DCM, "Reference Basis") = (88986008, SCT, "Vertex of Head") with EV (128773, DCM, "Reference Geometry") = (128120, DCM, "Plane through Superior Extent"), or EV (128772, DCM, "Reference Basis") = (56459004, SCT, "Foot") with EV (128773, DCM, "Reference Geometry") = (128121, DCM, "Plane through Inferior Extent")
Row 20 | This distance (likely recorded by the operator) locates the patient with respect to an X-Ray table landmark. The patient is assumed to be centered in the left-right axis of the X-Ray table.

Prev | Up | Next
X-Ray Radiation Dose SR IOD Templates | Home | TID 10003 Irradiation Event X-Ray Data

DICOM PS3.16 2020c - Content Mapping Resource