DICOM PS3.5 2020c - Data Structures and Encoding

A.9 SMPTE ST 2110-20 Uncompressed Interlaced Active Video Transfer Syntax (Current)
Prev | A Transfer Syntax Specifications (Normative) | Next

## A.9 SMPTE ST 2110-20 Uncompressed Interlaced Active Video Transfer Syntax

This Transfer Syntax is used in a DICOM-RTV Metadata Flow in order to describe the accompanying [SMPTE ST 2110-20] Video Flow.

The parameters are similar to the ones described in the [SMPTE ST 2110-20] Uncompressed Progressive Active Video ( label), but the frames are interlaced, one frame containing only odd lines and the next one containing only even lines.

A DICOM Transfer Syntax for SMPTE ST 2110-20 Uncompressed Interlaced Active Video shall be identified by a UID value of:

- 1.2.840.10008.1.2.7.2 corresponding to [SMPTE ST 2110-20] for the interlaced video.

Prev | Up | Next
A.8 SMPTE ST 2110-20 Uncompressed Progressive Active Video Transfer Syntax | Home | A.10 : SMPTE ST 2110-30 PCM Audio Transfer Syntax

DICOM PS3.5 2020c - Data Structures and Encoding