DICOM PS3.3 2020c - Information Object Definitions

A.34.5.4.6 Channel Source (Current)
Prev | A.34.5.4 Ambulatory ECG IOD Content Constraints | Next

##### A.34.5.4.6 Channel Source

For Channel Source Sequence (003A,0208) in each Channel Definition Sequence (003A,0200) Item DCID 3001 “ECG Leads” shall be used.

Prev | Up | Next
A.34.5.4.5 Sampling Frequency | Home | A.34.5.4.7 Waveform Sample Interpretation

DICOM PS3.3 2020c - Information Object Definitions