DICOM PS3.16 2020c - Content Mapping Resource

TID 3304 Stress Test Measurement Group (Current)
Prev | Stress Testing Report Templates | Next

### TID 3304 Stress Test Measurement Group

Each instance of the Stress Test Measurement Group represents a group of data elements acquired at approximately the same instant, and conventionally rendered as row in a tabular presentation. It is typically generated during the Stress exam whenever a time interval elapses (for example, every minute of the phase), when a technician observes data worth capturing, or when measurements exceed a given range.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3304. Stress Test Measurement Group

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | DT (59776-5, LN, "Findings") | 1 | M |  |
2 | > | CONTAINS | NUM | DT (252131008, SCT, "Time since start of exam") | 1 | M |  | UNITS = DT (min, UCUM, "min")
3 | > | CONTAINS | NUM | DT (122710, DCM, "Time since start of stage") | 1 | M |  | UNITS = DT (min, UCUM, "min")
4 | > | CONTAINS | NUM | DT (122702, DCM, "Treadmill speed") | 1 | U |  | UNITS = DCID 3212 “Treadmill Speed”
5 | > | CONTAINS | NUM | DT (122703, DCM, "Treadmill gradient") | 1 | U |  | UNITS = EV (%, UCUM, "%")
6 | > | CONTAINS | NUM | DT (122704, DCM, "Ergometer power") | 1 | U |  | UNITS = EV (W, UCUM, "Watts")
7 | > | CONTAINS | NUM | DT (122709, DCM, "Activity workload") | 1 | U |  | UNITS = DT ([MET], UCUM, "METS")
8 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DT (122706, DCM, "Rating of Perceived Exertion") $Method = BCID 3239 “Perceived Exertion Scales”
9 | > | CONTAINS | NUM | DT (122705, DCM, "Pharmacological Stress Agent Dose Rate") | 1 | MC | IFF Pharmacological Stress used | UNITS = EV (ug/kg/min, UCUM, "ug/kg/min")
10 | > | CONTAINS | INCLUDE | DTID 3106 “Drugs/Contrast Administered” | 1 | U |  |
11 | > | CONTAINS | NUM | EV (8867-4, LN, "Heart Rate") | 1 | U |  | UNITS = EV ({H.B.}/min, UCUM, "BPM")
12 | > | CONTAINS | NUM | EV (271649006, SCT, "Systolic Blood Pressure") | 1 | U |  | UNITS = DCID 3500 “Pressure Units”
13 | > | CONTAINS | NUM | EV (271650006, SCT, "Diastolic Blood Pressure") | 1 | U |  | UNITS = DCID 3500 “Pressure Units”
14 | > | CONTAINS | NUM | DT (122707, DCM, "Number of Ectopic Beats") | 1 | U |  | UNITS = EV ({beats}, UCUM, "beats")
15 | >> | HAS PROPERTIES | NUM | DT (260867005, SCT, "Period of collection") | 1 | M |  | UNITS = DT (min, UCUM, "min")
16 | >> | HAS PROPERTIES | CODE | EV (116676008, SCT, "Associated Morphology") | 1-n | U |  | BCID 3234 “Ectopic Beat Morphology”
17 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = DT (164931005, SCT, "ST Elevation") $Units = DT (mV, UCUM, "mV") $TargetSite = DCID 3001 “ECG Leads”
18 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = DT (429622005, SCT, "ST Depression") $Units = DT (mV, UCUM, "mV") $TargetSite = DCID 3001 “ECG Leads”
19 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = DCID 3228 “ECG Timing Measurements” $Units = DT (ms, UCUM, "ms") $TargetSite = DCID 3001 “ECG Leads”
20 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = DCID 3227 “QTc Measurements” $Units = DT (ms, UCUM, "ms") $TargetSite = DCID 3001 “ECG Leads” $Equation = DCID 3678 “QT Correction Algorithms”
21 | >> | INFERRED FROM | NUM | DT (2:16000, MDC, "RR Interval for QTc") | 1 | U |  | UNITS = DT (ms, UCUM, "ms")
22 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = DCID 3229 “ECG Axis Measurements” $Units = DT (deg, UCUM, "deg")
23 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3526 “Blood Gas Saturation” $Units = EV (%, UCUM, "%")
24 | > | CONTAINS | NUM | DT (122708, DCM, "Double Product") | 1 | U |  | UNITS = DT (mm[Hg].{H.B.}/min, UCUM, "mmHg.BPM")
25 | > | CONTAINS | CODE | EV (121071, DCM, "Finding") | 1-n | U |  | DCID 3220 “Stress Symptoms”
26 | > | CONTAINS | CODE | EV (271921002, SCT, "ECG Finding") | 1-n | U |  | DCID 3230 “ECG Findings”
27 | > | CONTAINS | TEXT | EV (121106, DCM, "Comment") | 1 | U |  |

Content Item Descriptions

Row 1 | The Container shall have a specific Content Item Observation DateTime (0040,A032) attribute to indicate the time at which the measurements were made.
Row 10 | Included TID 3106 “Drugs/Contrast Administered” allows the recording of test medications other than the Pharmacological Stress Agent identified in TID 3301 “Stress Test Procedure Description”.
Rows 17, 18 | ECG ST elevation/depression is measured in units of mV, but is conventionally reported in units of mm, based on strip recordings with scaling of 100 uV/mm. The display application should render these measurements in units meaningful to the user.
Row 19 | Note that the MDC codes for "per lead" measurements specified in CID 3228 “ECG Timing Measurements” are base codes for post-coordination with lead identifiers conveyed in the Target Site modifier in TID 300 “Measurement”. MDC also defines pre-coordinated codes that include both the measurement and the lead, which may be used in this row.
Row 20 | Note that the MDC code for "QTc interval per lead" specified in CID 3227 “QTc Measurements” is a base code for post-coordination with lead identifiers conveyed in the Target Site modifier in TID 300 “Measurement”. MDC also defines pre-coordinated codes that include both the measurement and the lead, which may be used in this row. Note that TID 300 “Measurement” enables the encoding of a non-standard correction algorithm, either as a local code, or as a TEXT Method Citation (see TID 300 “Measurement” row 12).
Row 21 | R-R interval used for QT correction algorithm
Row 22 | Recommended range for ECG axis measurements is -90° to +270°

Prev | Up | Next
TID 3303 Stress Test Phase Data | Home | TID 3307 NM/PET Perfusion Measurement Group

DICOM PS3.16 2020c - Content Mapping Resource