DICOM PS3.16 2020c - Content Mapping Resource

TID 10003C Irradiation Event X-Ray Mechanical Data (Current)
Prev | X-Ray Radiation Dose SR IOD Templates | Next

### TID 10003C Irradiation Event X-Ray Mechanical Data

This Template contains data that is expected to be available to the gantry or mechanical component of the equipment.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10003C. Irradiation Event X-Ray Mechanical Data

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (113956, DCM, "CR/DR Mechanical Configuration") | 1 | U |  | DCID 10031 “CR/DR Mechanical Configuration”
2 |  |  | NUM | EV (112011, DCM, "Positioner Primary Angle") | 1 | UC | XOR Row 6 | UNITS = EV (deg, UCUM, "deg")
3 |  |  | NUM | EV (112012, DCM, "Positioner Secondary Angle") | 1 | UC | XOR Row 6 | UNITS = EV (deg, UCUM, "deg")
4 |  |  | NUM | EV (113739, DCM, "Positioner Primary End Angle") | 1 | UC | IFF TID 10003 Row 7 value = (113613, DCM, "Rotational Acquisition") | UNITS = EV (deg, UCUM, "deg")
5 |  |  | NUM | EV (113740, DCM, "Positioner Secondary End Angle") | 1 | UC | IFF TID 10003 Row 7 value = (113613, DCM, "Rotational Acquisition") | UNITS = EV (deg, UCUM, "deg")
6 |  |  | NUM | EV (113770, DCM, "Column Angulation") | 1 | UC | XOR Rows 2, 3 | UNITS = EV (deg, UCUM, "deg")
7 |  |  | NUM | EV (113754, DCM, "Table Head Tilt Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
8 |  |  | NUM | EV (113755, DCM, "Table Horizontal Rotation Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
9 |  |  | NUM | EV (113756, DCM, "Table Cradle Tilt Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
10 |  |  | NUM | EV (111633, DCM, "Compression Thickness") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
10a |  |  | NUM | EV (111647, DCM, "Compression Force") | 1 | U |  | UNITS = EV (N, UCUM, "Newton")
10b |  |  | NUM | EV (111648, DCM, "Compression Pressure") | 1 | U |  | UNITS = EV (kPa, UCUM, "kilopascal")
10c |  |  | NUM | EV (111649, DCM, "Compression Contact Area") | 1 | U |  | UNITS = EV (mm2, UCUM, "mm2")
11 |  |  | NUM | DCID 10008 “Dose Related Distance Measurements” | 1-n | U |  | UNITS = EV (mm, UCUM, "mm")
12 |  |  | NUM | EV (128757, DCM, "Positioner Isocenter Primary Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
13 |  |  | NUM | EV (128758, DCM, "Positioner Isocenter Secondary Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
14 |  |  | NUM | EV (128759, DCM, "Positioner Isocenter Detector Rotation Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
15 |  |  | NUM | EV (128760, DCM, "Positioner Isocenter Primary End Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
16 |  |  | NUM | EV (128761, DCM, "Positioner Isocenter Secondary End Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
17 |  |  | NUM | EV (128762, DCM, "Positioner Isocenter Detector Rotation End Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
18 |  |  | NUM | EV (128763, DCM, "Table Head Tilt End Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
19 |  |  | NUM | EV (128764, DCM, "Table Horizontal Rotation End Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")
20 |  |  | NUM | EV (128765, DCM, "Table Cradle Tilt End Angle") | 1 | U |  | UNITS = EV (deg, UCUM, "deg")

Content Item Descriptions

Row 2 | Angle in patient's "equatorial" plane (LAO to RAO). For dynamically changing angle during the event, the start value shall be provided. Equivalent to (0018,1510) in an image instance.
Row 3 | Angle in patient's "sagittal" plane (CRAN to CAUD). For dynamically changing angle during the event, the start value shall be provided. Equivalent to (0018,1511) in an image instance.
Row 4 | In case of motion during irradiation event, Positioner Primary ending angle
Row 5 | In case of motion during irradiation event., Positioner Secondary ending angle
Row 6 | Column device Angle in equipment based coordinates
Rows 12 to 20 | Refer to the definitions of the X-Ray Isocenter Reference System (“X-Ray Isocenter Reference System Macro” in PS3.3 ).

Prev | Up | Next
TID 10003B Irradiation Event X-Ray Source Data | Home | TID 10004 Accumulated Fluoroscopy and Acquisition Projection X-Ray Dose

DICOM PS3.16 2020c - Content Mapping Resource