DICOM PS3.3 2020c - Information Object Definitions

C.8.27.4 Intravascular OCT Processing Parameters Module (Current)
Prev | C.8.27 Intravascular Optical Coherence Tomography Modules | Next

#### C.8.27.4 Intravascular OCT Processing Parameters Module

Table C.8.27.4-1 describes the parameters used for processing an Intravascular Optical Coherence Tomography polar data image.

Table C.8.27.4-1. Intravascular OCT Processing Parameters Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
OCT Z Offset Applied | (0052,0026) | 1 | Indicates whether or not Z offset correction was applied to the OCT image frames. Enumerated Values: YES NO
Refractive Index Applied | (0052,003A) | 1 | Indicates whether or not Refractive Index correction was applied. Enumerated Values: YES NO See Section C.8.27.4.1 for further explanation.
A-line Pixel Spacing | (0052,0014) | 1 | Spacing of pixels in the A-line (X-axis), in mm.
Pixel Intensity Relationship | (0028,1040) | 1 | The relationship between the pixel sample values and the IVOCT A-line intensity. See Section C.8.27.4.2.
First A-line Location | (0052,0034) | 1 | Orientation in degrees at which the 1st A-line in the frame should be displayed. Value shall be between 0 and 360, with zero representing vertical.

##### C.8.27.4.1 Refractive Index Applied

For Refractive Index Applied (0052,003A) a value of YES indicates that Effective Refractive Index (0052,0004) correction has been applied to the reported A-line Pixel Spacing (0052,0014) Attribute. A value of NO indicates that Effective Refractive Index (0052,0004) correction has not been applied (i.e., A-line Pixel Spacing corresponds to the pixel spacing in air).

###### C.8.27.4.2 Pixel Intensity Relationship

Pixel Intensity Relationship (0028,1040) shall identify the relationship of the pixel values to the IVOCT A-line intensity.

Defined Terms:

LIN

  Approximately proportional to A-line intensity.

LOG

  Non-linear "Log Function"; A Pixel Intensity Relationship LUT shall be included with the image to allow it to be scaled back to its proportional A-line intensity value.

Prev | Up | Next
C.8.27.3 Intravascular OCT Acquisition Parameters Module | Home | C.8.27.5 Intravascular Image Acquisition Parameters Module

DICOM PS3.3 2020c - Information Object Definitions