DICOM PS3.17 2020c - Explanatory Information

FFF.2.3.3 Pixel-shift (Current)
Prev | FFF.2.3 Display | Next

#### FFF.2.3.3 Pixel-shift

This section provides information on the Attribute encoding for use with image acquisitions that require subtracted display modes with multiple pixel shift ranges e.g., multiple subtracted views on a DSA acquisition.

##### FFF.2.3.3.1 User Scenario

When performing DSA acquisitions, the acquisition system may choose a default subtraction pixel-shift to allow review of the whole multi-frame, as acquired.

With advanced post-processing function the medical user may add further subtraction pixel-shifts to carve out certain details or improve contrast bolus visualization of a part of the anatomy that suffered from different movement during the acquisition.

Prev | Up | Next
FFF.2.3.2.4 Examples | Home | FFF.2.3.3.2 Encoding Outline

DICOM PS3.17 2020c - Explanatory Information