DICOM PS3.3 2020c - Information Object Definitions

A.34.17.4.5 Waveform Sample Interpretation (Current)
Prev | A.34.17.4 Body Position Waveform IOD Constraints | Next

##### A.34.17.4.5 Waveform Sample Interpretation

For channels encoding the patient's position as fixed values the value of Waveform Sample Interpretation (5400,1006) is UB.

For channels encoding the patient's position asrotation angles the value of Waveform Sample Interpretation (5400,1006) is SS.

Prev | Up | Next
A.34.17.4.4 Channel Source | Home | A.34.17.4.6 Waveform Data

DICOM PS3.3 2020c - Information Object Definitions