DICOM PS3.3 2020c - Information Object Definitions

C.8.19.4 X-Ray Image Intensifier Module (Current)
Prev | C.8.19 Enhanced XA/XRF Image | Next

#### C.8.19.4 X-Ray Image Intensifier Module

Table C.8.19.4-1 specifies the Attributes of the X-Ray Image Intensifier Module.

Table C.8.19.4-1. X-Ray Image Intensifier Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Intensifier Size | (0018,1162) | 1 | Physical diameter of the maximum active area X-Ray intensifier in mm. ### Note This Attribute does not specify the field of view. The Attribute Field of View Dimension(s) in Float (0018,9461) is intended for this value.
Intensifier Active Shape | (0018,9427) | 1 | Shape of the active area used for acquiring this image. Enumerated Values: RECTANGLE ROUND HEXAGONAL ### Note This may be different from the Field of View Shape (0018,1147), and should not be assumed to describe the stored image.
Intensifier Active Dimension(s) | (0018,9428) | 1 | Dimensions in mm of the active area used for acquiring this image. If Intensifier Active Shape (0018,9427) is: RECTANGLE: row dimension followed by column. ROUND: diameter. HEXAGONAL: diameter of the circle circumscribing the hexagon. ### Note This may be different from the Field of View Dimension(s) in Float (0018,9461), and should not be assumed to describe the stored image.

Prev | Up | Next
C.8.19.3 XA/XRF Acquisition Module | Home | C.8.19.5 X-Ray Detector Module

DICOM PS3.3 2020c - Information Object Definitions