DICOM PS3.3 2020c - Information Object Definitions

A.8.2 Multi-frame Single Bit Secondary Capture Image IOD (Current)
Prev | A.8 Secondary Capture Image IOD | Next

### A.8.2 Multi-frame Single Bit Secondary Capture Image IOD

#### A.8.2.1 Multi-frame Single Bit SC Image IOD Description

The Multi-frame Single Bit Secondary Capture (SC) Image Information Object Definition (IOD) specifies images that are converted from a non-DICOM format to a modality independent DICOM format.

This IOD is typically used for scanned documents and bitmap images of hand drawings.

Prev | Up | Next
A.8 Secondary Capture Image IOD | Home | A.8.2.2 Multi-frame Single Bit SC Image IOD Entity-Relationship Model

DICOM PS3.3 2020c - Information Object Definitions