DICOM PS3.3 2020c - Information Object Definitions

A.60.5 Visual Acuity Measurements IOD (Current)
Prev | A.60 Ophthalmic Refractive Measurements Information Object Definitions | Next

### A.60.5 Visual Acuity Measurements IOD

#### A.60.5.1 Visual Acuity Measurements IOD Description

The Visual Acuity Measurements IOD is used to capture a Patient's visual acuity relative to that of a reference standard Patient under given viewing conditions (distance, lighting, etc.).

Prev | Up | Next
A.60.4.3 Subjective Refraction Measurements IOD Module Table | Home | A.60.5.2 Visual Acuity Measurements IOD Entity-Relationship Model

DICOM PS3.3 2020c - Information Object Definitions