DICOM PS3.2 2020c - Conformance

M.4.4 Configuration (Current)
Prev | M Conformance Statement Sample DICOM-RTV Service Consumer (Informative) | Next

## M.4.4 Configuration

### M.4.4.1 DICOM-RTV Interface

The EXAMPLE-RTV-DISPLAY uses the network parameters (IP, portâ€¦) defined in the SDP.

Prev | Up | Next
M.4.3.3 IPv4 and IPv6 Support | Home | M.5 Media Interchange

DICOM PS3.2 2020c - Conformance