DICOM PS3.17 2020c - Explanatory Information

FFFF.3 Encoding Example (Current)
Prev | FFFF Advanced Blending Presentation State Storage Encoding Example (Informative) | Next

## FFFF.3 Encoding Example

Table FFFF.3-1. Encoding Example

Nesting | Attribute Name | Tag | Value | Comment
--- | --- | --- | --- | ---
| Advanced Blending Sequence | (0070,1B01) |  |
| %item 1 |  |  | Identifies Anatomical Series, no subset of series or registration
> | Blending Input Number | (0070,1B02) | 1 |
> | Study Instance UID | (0020,000D) | "1.3.46.670589.11.3" |
> | Series Instance UID | (0020,000E) | "1.3.46.670589.11.3.45" |
> | Geometry for Display | (0070,1B08) | TRUE | Series geometry shall be used as target geometry for the blending operation
| %enditem 1 |  |  |
| %item 2 |  |  | Identifies DTI Series, no subset of series is used, no registration present
> | Blending Input Number | (0070,1B02) | 2 |
> | Study Instance UID | (0020,000D) | "1.3.46.670589.11.3" |
> | Series Instance UID | (0020,000E) | "1.3.46.670589.11.3.49" |
> | Geometry for Display | (0070,1B08) | FALSE | Series geometry shall not be used as target geometry for the blending operation
| %enditem 2 |  |  |
| %item 3 |  |  | Identifies first Parametric map, no registration
> | Blending Input Number | (0070,1B02) | 3 |
> | Study Instance UID | (0020,000D) | "1.3.46.670589.11.3" |
> | Series Instance UID | (0020,000E) | "1.3.46.670589.11.3.56" |
> | Threshold Sequence | (0070,1B11) |  |
> | %item 3-1 |  |  |
>> | Threshold Value Sequence | (0070,1B12) |  |
>> | %item 3-1-1 |  |  |
>>> | Threshold Value | (0070,1B14) | 6 | First threshold value
>> | %enditem 3-1-1 |  |  |
>> | %item 3-1-2 |  |  |
>>> | Threshold Value | (0070,1B14) | 50 | Second threshold value
>> | %enditem 3-1-2 |  |  |
>> | Threshold Type | (0070,1B13) | RANGE_INCL |
> | %enditem 3-1 |  |  |
| %enditem 3 |  |  |
| %item 4 |  |  | Identifies second Parametric map, no registration
> | Blending Input Number | (0070,1B02) | 3 |
> | Study Instance UID | (0020,000D) | "1.3.46.670589.11.3" |
> | Series Instance UID | (0020,000E) | "1.3.46.670589.11.3.58" |
> | Threshold Sequence | (0070,1B11) |  |
> | %item 4-1 |  |  |
>> | Threshold Value Sequence | (0070,1B12) |  |
>>> | %item 4-1-1 |  |  |
>>> | Threshold Value | (0070,1B14) | 9 | First threshold value
>> | %enditem 4-1-1 |  |  |
>> | %item 4-1-2 |  |  |
>>> | Threshold Value | (0070,1B14) | 60 | Second threshold value
>> | %enditem 4-1-2 |  |  |
>> | Threshold Type | (0070,1B13) | RANGE_INCL |
> | %enditem 4-1 |  |  |
| %enditem 4 |  |  |
| %item 5 |  |  | Identifies third Parametric map, no registration
> | Blending Input Number | (0070,1B02) | 3 |
> | Study Instance UID | (0020,000D) | "1.3.46.670589.11.3" |
> | Series Instance UID | (0020,000E) | "1.3.46.670589.11.3.59" |
> | Threshold Sequence | (0070,1B11) |  |
> | %item 5-1 |  |  |
>> | Threshold Value Sequence | (0070,1B12) |  |
>> | %item 5-1-1 |  |  |
>>> | Threshold Value | (0070,1B14) | 7 | First threshold value
>> | %enditem 5-1-1 |  |  |
>> | %item 5-1-2 |  |  |
>>> | Threshold Value | (0070,1B14) | 75 | Second threshold value
>> | %enditem 5-1-2 |  |  |
>> | Threshold Type | (0070,1B13) | RANGE_INCL |
> | %enditem 5-1 |  |  |
| %enditem 5 |  |  |
| Pixel Presentation | (0008,9205) | "TRUE_COLOR" |
| Blending Display Sequence | (0070,1B04) |  |
| %item 1 |  |  |
> | Blending Display Input Sequence | (0070,1B03) |  |
> | %item 1-1 |  |  | Anatomical series, no threshold
>> | Blending Input Number | (0070,1B02) | 1 |
> | %enditem 1-1 |  |  |
> | %item 1-2 |  |  | DTI series, no threshold
>> | Blending Input Number | (0070,1B02) | 2 |
> | %enditem 1-2 |  |  |
> | Relative Opacity | (0070,0403) | 0.7 |
> | Blending Mode | (0070,1B06) | FOREGROUND |
> | Blending Input Number | (0070,1B02) | 6 | Output is used for later Blending
| %enditem 1 |  |  |
| %item 2 |  |  |
> | Blending Display Input Sequence | (0070,1B03) |  |
> | %item 2-1 |  |  | Parametric series 1
>> | Blending Input Number | (0070,1B02) | 3 |
> | %enditem 2-1 |  |  |
> | %item 2-2 |  |  | Parametric series 2
>> | Blending Input Number | (0070,1B02) | 4 |
> | %enditem 2-2 |  |  |
> | %item 2-3 |  |  | Parametric series 3
>> | Blending Input Number | (0070,1B02) | 5 |
> | End Sequence Item 2-3 |  |  |
> | Blending Mode | (0070,1B06) | EQUAL |
> | Blending Input Number | (0070,1B02) | 7 | Output is used for later Blending
| %enditem 2 |  |  |
| %item 3 |  |  |
> | Blending Display Input Sequence | (0070,1B03) |  |
> | %item 3-1 |  |  | Output first blending operation, no threshold
>> | Blending Input Number | (0070,1B02) | 6 |
> | %enditem 3-1 |  |  |
> | %item 3-2 |  |  | Output second blending operation, no threshold
>> | Blending Input Number | (0070,1B02) | 7 |
> | %enditem 3-2 |  |  |
> | Relative Opacity | (0070,0403) | 0.6 |
> | Blending Mode | (0070,1B06) | FOREGROUND |
| %enditem 3 |  |  | No Parametric Blending Input Number is present as this step defines the output to be displayed.

Prev | Up | Next
FFFF.2 Example | Home | GGGG Patient Radiation Dose Structured Report Document (Informative)

DICOM PS3.17 2020c - Explanatory Information