DICOM PS3.4 2020c - Service Class Specifications

R.3.3 Instance Availability Notification SOP Class UID (Current)
Prev | R.3 Instance Availability Notification SOP Class | Next

### R.3.3 Instance Availability Notification SOP Class UID

The Instance Availability Notification SOP Class shall be uniquely identified by the Instance Availability Notification SOP Class UID, which shall have the value "1.2.840.10008.5.1.4.33".

Prev | Up | Next
R.3.2 Operations | Home | R.3.4 Conformance Requirements

DICOM PS3.4 2020c - Service Class Specifications