DICOM PS3.18 2020c - Web Services

10.4.3.3 Response Payload (Current)
Prev | 10.4.3 Response | Next

#### 10.4.3.3 Response Payload

A success response shall have a payload containing one or more representations of the Target Resource in an Acceptable Media Type. The payload may be single part or multipart depending on the media type.

A failure response payload should contain a Status Report describing any failures, warnings, or other useful information.

Table 10.4.3-3 shows the media type category for each resource type. The origin server shall support the default and required media types in the media type category specified.

Table 10.4.3-3. Resource Media Types

Resource | Section | Media Type Category
--- | --- | ---
DICOM Resources | Section 10.4.1.1.1 | DICOM Media Types
Metadata Resources | Section 10.4.1.1.2 | DICOM Media Types
Rendered Resources | Section 10.4.1.1.3 | Rendered Media Types
Thumbnail Resources | Section 10.4.1.1.4 | Rendered Media Types

DICOM Media Types are described in Section 8.7.3. Rendered Media Types are described in Section 8.7.4.

Prev | Up | Next
10.4.3.2 Response Header Fields | Home | 10.4.4 Media Types

DICOM PS3.18 2020c - Web Services