DICOM PS3.17 2020c - Explanatory Information

PPP.3 Examples of Display System SOP Class (Current)
Prev | PPP Examples of Communication of Display Parameters (Informative) | Next

## PPP.3 Examples of Display System SOP Class

### PPP.3.1 An Example of A Typical Display System

A typical Display System is shown in Figure PPP.3.1-1.

Figure PPP.3.1-1. A Typical Display System

The following is an example of an N-GET Request/Response pair for the Display System SOP Class.

This example is encoded with Undefined Sequence Length and Undefined Item Length, so it contains Sequence Delimitation Items and Item Delimitation Items.

N-GET:

ANP

  Attribute Not Present.

VNP

  Attribute Present but Value Not Present.

-

  Not specified.

Table PPP.3.1-1. N-GET Request/Response Example

Attribute Name | Tag | N-GET Request (SCU) | N-GET Response (SCP)
--- | --- | --- | ---
SOP Common and Workstation Modules
Specific Character Set | (0008,0005) | ANP | \ISO 2022 IR 87
Manufacturer | (0008,0070) | VNP | NIPPON Corporation
Institution Name | (0008,0080) | VNP | JIRA Hospital
Institution Address | (0008,0081) | VNP | Bunkyo-ku, Tokyo, Japan
Device Serial Number | (0018,1000) | VNP | SN1234567890
Station Name | (0008,1010) | VNP | WorkstationX
Institutional Department Name | (0008,1040) | VNP | Radiology Dept.
Manufacturer's Model Name | (0008,1090) | VNP | QAStation-Model2013
Equipment Administrator Sequence | (0028,7000) | VNP |
>Item #1 of Equipment Administrator Sequence | (FFFE,E000) | - |
>Person Name | (0040,A123) | - | Yamada^Tarou=山田^太郎=やまだ^たろう
>Person Identification Code Sequence | (0040,1101) | - |
>>Item #1 of Person Identification Code Sequence | (FFFE,E000) | - |
>>Code Value | (0008,0110) | - | 111111
>>Coding Scheme Designator | (0008,0102) | - | LOCAL
>>Code Meaning | (0008,0104) | - | Yamada^Tarou
>>Item Delimiter of Item #1 of Person Identification Code Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Person Identification Code Sequence | (FFFE,E0DD) | - |
>Person's Address | (0040,1102) | - |
>Person's Telephone Number | (0040,1103) | - | EXT. 1234
>Institution Name | (0008,0080) | - | IT Support Div.
>Item Delimiter of Item #1 of Equipment Administrator Sequence | (FFFE,E00D) | - |
>Sequence Delimiter of Equipment Administrator Sequence | (FFFE,E0DD) | - |
Display System Module
Number of Display Subsystems | (0028,7001) |  | 3
Display Subsystem Sequence | (0028,7023) | VNP |
Item #1 of Display Subsystem Sequence | (FFFE,E000) | - |
>Display Subsystem ID | (0028,7003) | - | 1
>Display Subsystem Name | (0028,7004) | - | DSS1ofWSX
>Display Subsystem Description | (0028,7005) | - | For viewing a list and reports
>Display Device Type Code Sequence | (0028,7022) | - |
>>Item #1 of Display Device Type Code Sequence | (FFFE,E000) | - |
>>Code Value | (0008,0100) | - | 109992
>>Coding Scheme Designator | (0008,0102) | - | DCM
>>Code Meaning | (0008,0104) | - | Liquid Crystal Display
>>Item Delimiter of Item #1 of Display Device Type Code Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Device Type Code Sequence | (FFFE,E0DD) | - |
>Manufacturer | (0008,0070) | - | Color Monitor Corp.
>Device Serial Number | (0018,1000) | - | C201300011
>Manufacturer's Model Name | (0008,1090) | - | 1MC
> System Status | (0028,7006) | - | NORMAL
> System Status Comment | (0028,7007) | - |
>Display Subsystem Configuration Sequence | (0028,700A) | - |
>>Item #1 of Display Subsystem Configuration Sequence | (FFFE,E000) | - |
>> Configuration ID | (0028,700B) | - | 1
>> Configuration Name | (0028,700C) | - | DSS1Config1
>> Configuration Description | (0028,700D) | - | Configuration1 of Display Subsystem ID1
>>Referenced Target Luminance Characteristics ID | (0028,700E) | - | 1
>>Item Delimiter of Item #1 of Display Subsystem Configuration Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Subsystem Configuration Sequence | (FFFE,E0DD) | - |
>Current Configuration ID | (0028,7002) | - | 1
>Measurement Equipment Sequence | (0028,7012) | - |
>Sequence Delimiter of Measurement Equipment Sequence | (FFFE,E0DD) | - |
>Item Delimiter of Item #1 of Display System Sequence | (FFFE,E00D) | - |
>Item #2 of Display Subsystem Sequence | (FFFE,E000) | - |
>Display Subsystem ID | (0028,7003) | - | 2
>Display Subsystem Name | (0028,7004) | - | DSS2ofWSX
>Display Subsystem Description | (0028,7005) | - | Diagnostic, Monochrome
>Display Device Type Code Sequence | (0028,7022) | - |
>>Item #1 of Display Device Type Code Sequence | (FFFE,E00D) | - |
>>Code Value | (0008,0100) | - | 109992
>>Coding Scheme Designator | (0008,0102) | - | DCM
>>Code Meaning | (0008,0104) | - | Liquid Crystal Display
>>Item Delimiter of Display Device Type Code Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Device Type Code Sequence | (FFFE,E0DD) | - |
>Manufacturer | (0008,0070) | - | Medical Display Corp.
>Device Serial Number | (0018,1000) | - | 3M123456789
>Manufacturer's Model Name | (0008,1090) | - | 3MG
> System Status | (0028,7006) | - | NORMAL
> System Status Comment | (0028,7007) | - |
>Display Subsystem Configuration Sequence | (0028,700A) | - |
>>Item #1 of Display Subsystem Configuration Sequence | (FFFE,E000) | - |
>>Configuration ID | (0028,700B) | - | 1
>> Configuration Name | (0028,700C) | - | DSS2Config1
>> Configuration Description | (0028,700D) | - | Configuration2 of Display Subsystem ID2
>>Referenced Target Luminance Characteristics ID | (0028,700E) | - | 2
>>Item #1 of Display Subsystem Configuration Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Subsystem Configuration Sequence | (FFFE,E0DD) | - |
>Current Configuration ID | (0028,7002) | - | 1
>Measurement Equipment Sequence | (0028,7012) | - |
>>Item #1 of Measurement Equipment Sequence | (FFFE,E000) | - |
>>Measurement Functions | (0028,7013) | - | PHOTOMETER\COLORIMETER
>>Measured Characteristics | (0028,7026) | - | UNIFORMITY\LUMINANCE\CHROMATICITY
>>Measurement Equipment Type | (0028,7014) | - | BUILT_IN_FRONT
>> Manufacturer | (0008,0070) | - | LuminanceMeasurement Device Inc.
>> Manufacturer's Model Name | (0008,1090) | - | LC1000
>> Device Serial Number | (0018,1000) | - | SN99990001
>> DateTime of Last Calibration | (0018,1202) | - |
>>Item Delimiter of Item #1 of Measurement Equipment Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Measurement Equipment Sequence | (FFFE,E0DD) | - |
>Item Delimiter of Item #2 of Display Subsystem Sequence | (FFFE,E00D) | - |
>Item #3 of Display Subsystem Sequence | (FFFE,E000) | - |
>Display Subsystem ID | (0028,7003) | - | 3
>Display Subsystem Name | (0028,7004) | - | DSS3ofWSX
>Display Subsystem Description | (0028,7005) | - | Diagnostic, Monochrome
>Display Device Type Code Sequence | (0028,7022) | - |
>>Item #1 of Display Device Type Code Sequence | (FFFE,E000) | - |
>>Code Value | (0008,0100) | - | 109992
>>Coding Scheme Designator | (0008,0102) | - | DCM
>>Code Meaning | (0008,0104) | - | Liquid Crystal Display
>>Item Delimiter of Item #1 of Display Device Type Code Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Device Type Code Sequence | (FFFE,E0DD) | - |
>Manufacturer | (0008,0070) | - | Medical Display Corp.
>Device Serial Number | (0018,1000) | - | 3M123456790
>Manufacturer's Model Name | (0008,1090) | - | 3MG
>System Status | (0028,7006) | - | NORMAL
>System Status Comment | (0028,7007) | - |
> Display Subsystem Configuration Sequence | (0028,700A) | - |
>>Item #1 of Display Subsystem Configuration Sequence | (FFFE,E000) | - |
>> Configuration ID | (0028,700B) | - | 1
>> Configuration Name | (0028,700C) | - | DSS3Config1
>> Configuration Description | (0028,700D) | - | Configuration3 of Display Subsystem ID3
>>Referenced Target Luminance Characteristics ID | (0028,700E) | - | 3
>>Item Delimiter of Item #1 of Display Subsystem Configuration Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Subsystem Configuration Sequence | (FFFE,E0DD) | - |
>Current Configuration ID | (0028,7002) | - | 1
>Measurement Equipment Sequence | (0028,7012) | - |
>>Item #1 of Measurement Equipment Sequence | (FFFE,E000) | - |
>>Measurement Functions | (0028,7013) | - | PHOTOMETER\COLORIMETER
>>Measured Characteristics | (0028,7026) | - | UNIFORMITY\LUMINANCE\CHROMATICITY
>>Measurement Equipment Type | (0028,7014) | - | BUILT_IN_FRONT
>> Manufacturer | (0008,0070) | - | LuminanceMeasurement Device Inc.
>>Manufacturer's Model Name | (0008,1090) | - | LC1000
>> Device Serial Number | (0018,1000) | - | SN99990011
>> DateTime of Last Calibration | (0018,1202) | - |
>>Item Delimiter of Item #1 of Measurement Equipment Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Measurement Equipment Sequence | (FFFE,E0DD) | - |
>Item Delimiter of Item #3 of Display Subsystem Sequence | (FFFE,E00D) | - |
>Sequence Delimiter of Display Subsystem Sequence | (FFFE,E0DD) | - |
Target Luminance Characteristics Module
Target Luminance Characteristics Sequence | (0028,7008) | VNP |
>Item #1 of Target Luminance Characteristics Sequence | (FFFE,E000) | - |
>Luminance Characteristics ID | (0028,7009) | - | 1
>Display Function Type | (0028,7019) | - | GAMMA
>Target Minimum Luminance | (0028,701D) | - | 0.75
>Target Maximum Luminance | (0028,701E) | - | 250
>Gamma Value | (0028,701A) | - | 2.2
>Item Delimiter of Item #1 of Target Luminance Characteristics Sequence | (FFFE,E00D) | - |
>Item #2 of Target Luminance Characteristics Sequence | (FFFE,E000) | - |
>Luminance Characteristics ID | (0028,7009) | - | 2
>Display Function Type | (0028,7019) | - | GSDF
>Target Minimum Luminance | (0028,701D) | - | 0.75
>Target Maximum Luminance | (0028,701E) | - | 521.0
>Reflected Ambient Light | (2010,0160) | - | 0.410
>Ambient Light Value Source | (0028,7025) | - | DEFAULT
>Item Delimiter of Item #2 of Target Luminance Characteristics Sequence | (FFFE,E00D) | - |
>Item #3 of Target Luminance Characteristics Sequence | (FFFE,E000) | - |
>Luminance Characteristics ID | (0028,7009) | - | 3
>Display Function Type | (0028,7019) | - | GSDF
>Target Minimum Luminance | (0028,701D) | - | 0.75
>Target Maximum Luminance | (0028,701E) | - | 520.0
>Reflected Ambient Light | (2010,0160) | - | 0.410
>Ambient Light Value Source | (0028,7025) | - | DEFAULT
>Item Delimiter of Item #3 of Target Luminance Characteristics Sequence | (FFFE,E00D) | - |
>Sequence Delimiter of Target Luminance Characteristics Sequence | (FFFE,E0DD) | - |
QA Result Module
See Table PPP.3.1-2.

This example is encoded with Undefined Sequence Length and Undefined Item Length , so it contains Sequence Delimitation Items and Item Delimitation Items.

Table PPP.3.1-2. Example of N-GET Request/Response for QA Result Module

Attribute Name | Tag | N-GET Request (SCU) | N-GET Response (SCP)
--- | --- | --- | ---
QA Result Module
QA Results Sequence | (0028,700F) | VNP |
>Item #1 of QA Results Sequence | (FFFE,E000) | - |
>Display Subsystem ID | (0028,7003) | - | 2
>Display Subsystem QA Results Sequence | (0028,7010) | - |
>>Item #1 of Display System QA Results Sequence | (FFFE,E000) | - |
>>Configuration ID | (0028,700B) | - | 1
>>Configuration QA Results Sequence | (0028,7011) | - |
>>>Item #1 of Configuration QA Results Sequence | (FFFE,E000) | - |
>>>Display Calibration Result Sequence | (0028,7016) | - |
>>>>Item #1 of Display Calibration Result Sequence |  | - |
>>>>Performed Procedure Step Start DateTime | (0040,4050) | - | 20130610191010
>>>>Performed Procedure Step End DateTime | (0040,4051) | - | 20130610192030
>>>>Actual Human Performer Sequence | (0040,4035) | - |
>>>>Item #1 of Actual Human Performer Sequence | (FFFE,E000) | - |
>>>>>Human Performer's Name | (0040,4037) | - | Kido^Kousei
>>>>>Human Performer's Organization | (0040,4036) | - | QA Dept.
>>>>> Item Delimiter of Item #1 of Actual Human Performer Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Actual Human Performer Sequence | (FFFE,E0DD) | - |
>>>>Measurement Equipment Sequence | (0028,7012) | - |
>>>>>Item #1 of Measurement Equipment Sequence | (FFFE,E000) | - |
>>>>>Measurement Functions | (0028,7013) | - | PHOTOMETER
>>>>>Measured Characteristics | (0028,7026) | - | LUMINANCE
>>>>>Measurement Equipment Type | (0028,7014) | - | NEAR_RANGE
>>>>>Manufacturer | (0008,0070) | - | LUXDEVICE COMPANY
>>>>>Manufacturer's Model Name | (0008,1090) | - | PHOTOMETER MODEL1
>>>>>Device Serial Number | (0018,1000) | - | PM1-141421356
>>>>>DateTime of Last Calibration | (0018,1202) | - | 201303310900
>>>>> Item Delimiter of Item #1 of Measurement Equipment Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Measurement Equipment Sequence | (FFFE,E0DD) | - |
>>>>Luminance Characteristics ID | (0028,7009) | - | 2
>>>>Item #1 of Display Calibration Result Sequence | (FFFE,E00D) | - |
>>>>Sequence Delimiter of Display Calibration Result Sequence | (FFFE,E0DD) | - |
>>>Visual Evaluation Result Sequence | (0028,7015) | - |
>>>>Item #1 of Visual Evaluation Result Sequence | (FFFE,E000) | - |
>>>>Performed Procedure Step Start DateTime | (0040,4050) | - | 201307150900
>>>>Performed Procedure Step End DateTime | (0040,4051) | - | 201307150910
>>>>Actual Human Performer Sequence | (0040,4035) | - |
>>>>Item #1 of Actual Human Performer Sequence | (FFFE,E000) | - |
>>>>>Human Performer's Name | (0040,4037) | - | Mokushi^Shirou
>>>>>Human Performer's Organization | (0040,4036) | - | Radiology Dept.
>>>>> Item Delimiter of Item #1 of Actual Human Performer Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Actual Human Performer Sequence | (FFFE,E0DD) | - |
>>>>Visual Evaluation Test Sequence | (0028,7028) | - |
>>>>>Item #1 of Visual Evaluation Test Sequence | (FFFE,E000) | - |
>>>>>Test Result | (0028,7029) | - | PASS
>>>>>Test Result Comment | (0028,702A) | - | All appearances were OK.
>>>>>Test Pattern Code Sequence | (0028,702C) | - |
>>>>>>Item #1 of Test Pattern Code Sequence | (FFFE,E000) | - |
>>>>>>Code Value | (0008,0100) | - | 109801
>>>>>>Coding Scheme Designator | (0008,0102) | - | DCM
>>>>>>Code Meaning | (0008,0104) | - | TG18-QC Pattern
>>>>>> Item Delimiter of Item #1 of Test Pattern Code Sequence | (FFFE,E00D) | - |
>>>>>>Sequence Delimiter of Test Pattern Code Sequence | (FFFE,E0DD) | - |
>>>>>Visual Evaluation Method Code Sequence | (0028,702E) | - |
>>>>>>Item #1 of Visual Evaluation Method Code Sequence | (FFFE,E000) | - |
>>>>>>Code Value | (0008,0100) | - | 109701
>>>>>>Coding Scheme Designator | (0008,0102) | - | DCM
>>>>>>Code Meaning | (0008,0104) | - | Overall image quality evaluation
>>>>>> Item Delimiter of Item #1 of Visual Evaluation Method Code Sequence | (FFFE,E00D) | - |
>>>>>>Sequence Delimiter of Visual Evaluation Method Code Sequence | (FFFE,E0DD) | - |
>>>> Item Delimiter of Item #1 of Visual Evaluation Test Sequence | (FFFE,E00D) | - |
>>>Sequence Delimiter of Visual Evaluation Test Sequence | (FFFE,E0DD) | - |
>>>Luminance Uniformity Result Sequence | (0028,7027) | - |
>>>>Item #1 of Luminance Uniformity Result Sequence | (FFFE,E000) | - |
>>>>Performed Procedure Step Start DateTime | (0040,4050) | - | 20130610195000
>>>>Performed Procedure Step End DateTime | (0040,4051) | - | 20130610195900
>>>>Actual Human Performer Sequence | (0040,4035) | - |
>>>>Item #1 of Actual Human Performer Sequence | (FFFE,E000) | - |
>>>>>Human Performer's Name | (0040,4037) | - | Kido^Kousei
>>>>>Human Performer's Organization | (0040,4036) | - | QA Dept.
>>>>>Item Delimiter of Item #1 of Actual Human Performer Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Actual Human Performer Sequence | (FFFE,E0DD) | - |
>>>>Measurement Equipment Sequence | (0028,7012) | - |
>>>>>Item #1 of Measurement Equipment Sequence | (FFFE,E000) | - |
>>>>>Measurement Functions | (0028,7013) | - | PHOTOMETER\COLORIMETER
>>>>>Measured Characteristics | (0028,7026) | - | LUMINANCE\CHROMATICITY
>>>>>Measurement Equipment Type | (0028,7014) | - | NEAR_RANGE
>>>>>Manufacturer | (0008,0070) | - | LUXDEVICE COMPANY
>>>>>Manufacturer's Model Name | (0008,1090) | - | PHOTOMETER MODEL1
>>>>>Device Serial Number | (0018,1000) | - | PM1-141421356
>>>>>DateTime of Last Calibration | (0018,1202) | - | 201303310900
>>>>>Item Delimiter of Item #1 of Measurement Equipment Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Measurement Equipment Sequence | (FFFE,E0DD) | - |
>>>>Number of Luminance Points | (0028,701B) | - | 5
>>>>Measurement Pattern Code Sequence | (0028,702D) | - |
>>>>>Item #1 of Measurement Pattern Code Sequence | (FFFE,E000) | - |
>>>>>Code Value | (0008,0100) | - | 109844
>>>>>Coding Scheme Designator | (0008,0102) | - | DCM
>>>>>Code Meaning | (0008,0104) | - | TG18-UNL80 Pattern
>>>>>Item Delimiter of Item #1 of Measurement Pattern Code Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Measurement Pattern Code Sequence | (FFFE,E0DD) | - |
>>>>DDL Value | (0028,7017) | - | 204
>>>>White Point Flag | (0028,7021) | - | YES
>>>>Luminance Response Sequence | (0028,701C) | - |
>>>>>Item #1 of Luminance Response Sequence | (FFFE,E000) | - |
>>>>>Luminance Value | (0028,701F) | - | 191.5
>>>>>CIExy White Point | (0028,7018) | - | 0.940694\1.455249
>>>>>Item Delimiter of Item #1Luminance Response Sequence | (FFFE,E00D) | - |
>>>>>Item #2 of Luminance Response Sequence | (FFFE,E000) | - |
>>>>>Luminance Value | (0028,701F) | - | 176.1
>>>>>CIExy White Point | (0028,7018) | - | 0.932555\1.421037
>>>>>Item Delimiter of Item #2 Luminance Response Sequence | (FFFE,E00D) | - |
>>>>>Item #3 of Luminance Response Sequence | (FFFE,E000) | - |
>>>>>Luminance Value | (0028,701F) | - | 197.2
>>>>>CIExy White Point | (0028,7018) | - | 0.918886\1.416465
>>>>>Item Delimiter of Item #3 of Luminance Response Sequence | (FFFE,E00D) | - |
>>>>>Item #4 of Luminance Response Sequence | (FFFE,E000) | - |
>>>>>Luminance Value | (0028,701F) | - | 202.5
>>>>>CIExy White Point | (0028,7018) | - | 0.940709\1.434902
>>>>>Item Delimiter of Item #4 Luminance Response Sequence | (FFFE,E00D) | - |
>>>>>Item #5 of Luminance Response Sequence | (FFFE,E000) | - |
>>>>>Luminance Value | (0028,701F) | - | 195.8
>>>>>CIExy White Point | (0028,7018) | - | 0.946154\1.477551
>>>>>Item Delimiter of Item #5Luminance Response Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Luminance Response Sequence | (FFFE,E0DD) | - |
>>>Luminance Result Sequence | (0028,7024) | - |
>>>>Item #1 of Luminance Result Sequence | (0028,e000) | - |
>>>>Performed Procedure Step Start DateTime | (0040,4050) | - | 20130610194000
>>>>Performed Procedure Step End DateTime | (0040,4051) | - | 20130610195500
>>>>Actual Human Performer Sequence | (0040,4035) | - |
>>>>Item #1 of Actual Human Performer Sequence | (FFFE,E000) | - |
>>>>>Human Performer's Name | (0040,4037) | - | Kido^Kousei
>>>>>Human Performer's Organization | (0040,4036) | - | QA Dept.
>>>>>Item Delimiter of Item #1 of Actual Human Performer Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Actual Human Performer Sequence | (FFFE,E0DD) | - |
>>>>Measurement Equipment Sequence | (0028,7012) | - |
>>>>>Item #1 of Measurement Equipment Sequence | (FFFE,E000) | - |
>>>>>Measurement Functions | (0028,7013) | - | PHOTOMETER\COLORIMETER
>>>>>Measured Characteristics | (0028,7026) | - | LUMINANCE\CHROMATICITY
>>>>>Measurement Equipment Type | (0028,7014) | - | NEAR_RANGE
>>>>>Manufacturer | (0008,0070) | - | LUXDEVICE COMPANY
>>>>>Manufacturer's Model Name | (0008,1090) | - | PHOTOMETER MODEL1
>>>>>Device Serial Number | (0018,1000) | - | PM1-141421356
>>>>>DateTime of Last Calibration | (0018,1202) | - | 201303310900
>>>>>Item Delimiter of Item #1 of Measurement Equipment Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Measurement Equipment Sequence | (FFFE,E0DD) | - |
>>>>Number of Luminance Points | (0028,701B) | - | 18
>>>>Luminance Response Sequence | (0028,701C) | - |
>>>>>Item #1 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 0
>>>>>Luminance Value | (0028,701F) | - | 0.64
>>>>>Item Delimiter of Item #1 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #2 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 15
>>>>>Luminance Value | (0028,701F) | - | 2.03
>>>>>Item Delimiter of Item #2 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #3 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 30
>>>>>Luminance Value | (0028,701F) | - | 4.17
>>>>>Item Delimiter of Item #3 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #4 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 45
>>>>>Luminance Value | (0028,701F) | - | 7.11
>>>>>Item Delimiter of Item #4 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #5 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 60
>>>>>Luminance Value | (0028,701F) | - | 11.12
>>>>>Item Delimiter of Item #5 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #6 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 75
>>>>>Luminance Value | (0028,701F) | - | 16.75
>>>>>Item Delimiter of Item #6 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #7 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 90
>>>>>Luminance Value | (0028,701F) | - | 24.07
>>>>>Item Delimiter of Item #7 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #8 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 105
>>>>>Luminance Value | (0028,701F) | - | 33.67
>>>>>Item Delimiter of Item #8 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #9 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 120
>>>>>Luminance Value | (0028,701F) | - | 46.24
>>>>>Item Delimiter of Item #9 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #10 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 135
>>>>>Luminance Value | (0028,701F) | - | 63.12
>>>>>Item Delimiter of Item #10 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #11 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 150
>>>>>Luminance Value | (0028,701F) | - | 83.94
>>>>>Item Delimiter of Item #11 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #12 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 160
>>>>>Luminance Value | (0028,701F) | - | 110.6
>>>>>Item Delimiter of Item #12 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #13 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 180
>>>>>Luminance Value | (0028,701F) | - | 144.9
>>>>>Item Delimiter of Item #13 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #14 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 195
>>>>>Luminance Value | (0028,701F) | - | 190.1
>>>>>Item Delimiter of Item #14 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #15 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 210
>>>>>Luminance Value | (0028,701F) | - | 246.3
>>>>>Item Delimiter of Item #15 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #16 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 225
>>>>>Luminance Value | (0028,701F) | - | 317.8
>>>>>Item Delimiter of Item #16 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #17 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 240
>>>>>Luminance Value | (0028,701F) | - | 406.4
>>>>>Item Delimiter of Item #17 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Item #18 of Luminance Result Sequence | (FFFE,E000) | - |
>>>>>DDL Value | (0028,7017) | - | 255
>>>>>Luminance Value | (0028,701F) | - | 520.9
>>>>>Item Delimiter of Item #18 of Luminance Result Sequence | (FFFE,E00D) | - |
>>>>>Sequence Delimiter of Luminance Response Sequence | (FFFE,E0DD) | - |
>>>>Reflected Ambient Light | (2010,0160) | - | 0.408
>>>>Ambient Light Source | (0028,7025) | - | MEASURED
>>>>Item Delimiter of Item #1 of Luminance Result Sequence | (0028,e00D) | - |
>>>>Sequence Delimiter of Luminance Result Sequence | (0028,e0DD) | - |
>>>Item #1 Configuration QA Results Sequence | (0028,e00D) | - |
>>>Sequence Delimiter of Configuration QA Results Sequence | (0028,e0DD) | - |
>>Item Delimiter of Item #1 of Display System QA Results Sequence | (0028,e00D) | - |
>Sequence Delimiter of Display System QA Results Sequence | (0028,e0DD) | - |
>Item Delimiter of Item #1 of QA Results Sequence | (0028,e00D) | - |
>Item #2 of QA Results Sequence | (FFFE,E000) | - |
>Display Subsystem ID | (0028,7003) | - | 3
… |  | - | The SCP will return the values for Display Subsystem ID=3.
>Item Delimiter of Item #2 of QA Results Sequence | (0028,e00D) | - |
>Sequence Delimiter of QA Results Sequence | (0028,e0DD) | - |

Prev | Up | Next
PPP.2 Examples of Message Sequencing | Home | PPP.3.2 An Example of A Tablet Display

DICOM PS3.17 2020c - Explanatory Information