DICOM PS3.17 2020c - Explanatory Information

S.5 Adding The First Managed Device to A Legacy Network (Current)
Prev | S Legacy Transition For Configuration Management (Informative) | Next

## S.5 Adding The First Managed Device to A Legacy Network

The addition of the first fully managed device to a legacy network requires both server setup and device setup.

### S.5.1 New Servers Required

The managed node requires that servers be installed or assigned to provide the following actors:

1. DHCP Server

2. DNS Server

3. NTP Server

4. LDAP Server

These may be existing servers that need only administrative additions, they may be existing hardware that has new software added, and these may be one or multiple different systems. DHCP, DNS, and NTP services are provided by a very wide variety of equipment.

Prev | Up | Next
S.4 Partially Managed Devices | Home | S.5.2 NTP

DICOM PS3.17 2020c - Explanatory Information