DICOM PS3.3 2020c - Information Object Definitions

A.34.16.4 Multi-channel Respiratory Waveform IOD Constraints (Current)
Prev | A.34.16 Multi-channel Respiratory Waveform IOD | Next

#### A.34.16.4 Multi-channel Respiratory Waveform IOD Constraints

##### A.34.16.4.1 Modality

The value of Modality (0008,0060) shall be RESP.

Prev | Up | Next
A.34.16.3 Multi-channel Respiratory Waveform IOD Module Table | Home | A.34.16.4.2 Waveform Sequence and Number of Waveform Channels

DICOM PS3.3 2020c - Information Object Definitions