DICOM PS3.3 2020c - Information Object Definitions

A.48.3 Enhanced XRF Image IOD Module Table (Current)
Prev | A.48 Enhanced XRF Image IOD | Next

### A.48.3 Enhanced XRF Image IOD Module Table

Table A.48-1 specifies the Modules of the Enhanced XRF Image IOD.

Table A.48-1. Enhanced XRF Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
XA/XRF Series | C.8.19.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | U
Synchronization | C.7.4.2 | U
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | Image Pixel | C.7.6.3 | M
Enhanced Contrast/Bolus | C.7.6.4b | C - Required if contrast media was applied and the system is able to register contrast usage.
Mask | C.7.6.10 | U
Device | C.7.6.12 | U
Intervention | C.7.6.13 | U
Acquisition Context | C.7.6.14 | M
Multi-frame Functional Groups | C.7.6.16 | M
Multi-frame Dimension | C.7.6.17 | U
Cardiac Synchronization | C.7.6.18.1 | C - Required if cardiac synchronization was applied.
Respiratory Synchronization | C.7.6.18.2 | C - Required if respiratory synchronization was applied.
Specimen | C.7.6.22 | U
X-Ray Tomography Acquisition | C.8.7.7 | U
X-Ray Filtration | C.8.7.10 | U
X-Ray Grid | C.8.7.11 | U
Enhanced XA/XRF Image | C.8.19.2 | M
XA/XRF Acquisition | C.8.19.3 | C - Required if Image Type (0008,0008) Value 1 equals ORIGINAL. May be present otherwise.
X-Ray Image Intensifier | C.8.19.4 | C - Required if X-Ray Receptor Type (0018,9420) is present and equals IMG_INTENSIFIER.
X-Ray Detector | C.8.19.5 | C - Required if X-Ray Receptor Type (0018,9420) is present and equals DIGITAL_DETECTOR.
XA/XRF Multi-frame Presentation | C.8.19.7 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

#### A.48.3.1 Enhanced XRF Image IOD Content Constraints

##### A.48.3.1.1 Modality Attribute

Modality (0008,0060) shall have the value RF.

##### A.48.3.1.2 Overlay Plane, Curve, VOI LUT and Specimen Identification Modules

The Overlay Plane Module, VOI LUT Module and Softcopy Presentation LUT Module shall not be used in a Standard Extended SOP Class of the Enhanced XRF Image.

### Note

1. The VOI LUT function is provided by a Frame VOI LUT Functional Group.

2. The Curve Module (Retired) was previously include in the list of Modules that shall not be present, but has been retired from DICOM. It is still not permitted to be present. See PS3.3-2004.

3. The Specimen Identification Module was previously included in this IOD but has been retired, and its functionality replaced by the Specimen Module. See PS3.3-2008.

##### A.48.3.1.3 Positioner Type

Positioner Type (0018,1508) shall have the value COLUMN if the XA/XRF Acquisition Module is present.

Prev | Up | Next
A.48.2 Enhanced XRF Image IOD Entity-Relationship Model | Home | A.48.4 Enhanced XRF Image Functional Group Macros

DICOM PS3.3 2020c - Information Object Definitions