DICOM PS3.17 2020c - Explanatory Information

PPP.2 Examples of Message Sequencing (Current)
Prev | PPP Examples of Communication of Display Parameters (Informative) | Next

## PPP.2 Examples of Message Sequencing

This section provides an examples of message sequencing when using the Display System SOP Class. This section is not intended to provide an exhaustive set of use cases but rather an informative example. There are other valid message sequences that could be used to obtain an equivalent outcome.

### PPP.2.1 Example of Retrieval of Status and Configuration From Display Systems

Figure PPP.2.1-1. Example of System Status and Configuration Message Sequencing

QC Management Station : Manages display systems status and Configurations. This works as an SCU.

Display System A and B : Have display devices. Each display device may be other display vendors'. These work as SCPs.

Generation and notification of change events are out of a scope of DICOM.

Prev | Up | Next
PPP Examples of Communication of Display Parameters (Informative) | Home | PPP.3 Examples of Display System SOP Class

DICOM PS3.17 2020c - Explanatory Information