DICOM PS3.17 2020d - Explanatory Information

TTT.2.2.2 Encoding Outline (Current)
Prev | TTT.2.2 Case #2: Reconstruction From A Sub-set of Projection Frames | Next

#### TTT.2.2.2 Encoding Outline

Only selected frames of the original XA instance or Enhanced XA instance are used to reconstruct the volume.

The X-Ray 3D instance references the original XA instance or Enhanced XA instance and uses Attributes to define the context on how and which of the original image frames are used to create the volume.

Figure TTT.2.2-1. Encoding of one 3D reconstruction from a sub-set of projection frames

Prev | Up | Next
TTT.2.2 Case #2: Reconstruction From A Sub-set of Projection Frames | Home | TTT.2.2.3 Encoding Details

DICOM PS3.17 2020d - Explanatory Information