DICOM PS3.17 2020d - Explanatory Information

TTT.2.5.3 Encoding Details (Current)
Prev | TTT.2.5 Case #5: One Rotation, One 2D Instance, Multiple Reconstructions, One X-Ray 3D Instance | Next

#### TTT.2.5.3 Encoding Details

##### TTT.2.5.3.1 2D X-Ray Angiographic Image IOD

This scenario is based on the encoding of a single rotational acquisition in one 2D instance, together with the information of the ECG and/or the cardiac trigger delay times of each frame of the rotational image.

Prev | Up | Next
TTT.2.5.2 Encoding Outline | Home | TTT.2.5.3.2 X-Ray 3D Angiographic Image IOD

DICOM PS3.17 2020d - Explanatory Information